### BB_BLEMPRIO1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:28 | RW | BLEM15 | Set priority value for passive extended passive scanning on secondary advertising channels
27:24 | RW | BLEM14 | Set priority value for non-connectable extended advertising on secondary advertising channels
23:20 | RW | BLEM13 | Set priority value for connectable extended advertising on secondary advertising channels
19:16 | RW | BLEM12 | Set priority value for extended active scanning on secondary advertising channels
15:12 | RW | BLEM11 | Set priority value for extended initiating on secondary advertising channels
11:8 | RW | BLEM10 | Set priority value for connection establishment BLE message on secondary advertising channels
7:4 | RW | BLEM9 | Set default priority value for ISO channel subsequent Tx/Rx attempt
3:0 | RW | BLEM8 | Set default priority value for ISO channel first Tx/Rx attempt

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:28 | BLEM15 | BLEM15_3 |  | 0x3*
27:24 | BLEM14 | BLEM14_4 |  | 0x4*
23:20 | BLEM13 | BLEM13_8 |  | 0x8*
19:16 | BLEM12 | BLEM12_9 |  | 0x9*
15:12 | BLEM11 | BLEM11_10 |  | 0xA*
11:8 | BLEM10 | BLEM10_15 |  | 0xF*
7:4 | BLEM9 | BLEM9_13 |  | 0xD*
3:0 | BLEM8 | BLEM8_12 |  | 0xC*