### SYSCTRL_NS_ACCESS_RAM_CFG1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
1:0 | RW | BB_DRAM_ACCESS | Allow Non-Secure code to access BB_DRAM[1:0]

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
1:0 | BB_DRAM_ACCESS | NS_CANNOT_ACCESS_BB_DRAM0 | Non-Secure code cannot access the BB_DRAM0 | 0x0*
|  | NS_CANNOT_ACCESS_BB_DRAM1 | Non-Secure code cannot access the BB_DRAM1 | 0x0*
|  | NS_CAN_ACCESS_BB_DRAM0 | Non-Secure code can access the BB_DRAM0 | 0x1
|  | NS_CAN_ACCESS_BB_DRAM1 | Non-Secure code can access the BB_DRAM1 | 0x2