### BB_RADIOPWRUPDN0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | SYNC_POSITION0 | Access address detection pulse/level position for uncoded PHY at 1Mbps
23:16 | RW | RXPWRUP0 | Radio Rx power up (in us) for uncoded PHY at 1Mbps
14:8 | RW | TXPWRDN0 | Radio Tx power down (in us) for uncoded PHY at 1Mbps
7:0 | RW | TXPWRUP0 | Radio Tx power up (in us) for uncoded PHY at 1Mbps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | SYNC_POSITION0 | SYNC_POSITION0_0 |  | 0x0*
23:16 | RXPWRUP0 | RXPWRUP0_0 |  | 0x0*
14:8 | TXPWRDN0 | TXPWRDN0_0 |  | 0x0*
7:0 | TXPWRUP0 | TXPWRUP0_0 |  | 0x0*