### ASCC_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
3:0 | RW | PERIODS_CFG | Defines over how many asynchronous clock periods the period counter measures

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
3:0 | PERIODS_CFG | ASCC_PERIODS_1 | Measure 1 asynchronous clock period | 0x0*
|  | ASCC_PERIODS_2 | Measure 2 asynchronous clock periods | 0x1
|  | ASCC_PERIODS_3 | Measure 3 asynchronous clock periods | 0x2
|  | ASCC_PERIODS_4 | Measure 4 asynchronous clock periods | 0x3
|  | ASCC_PERIODS_5 | Measure 5 asynchronous clock periods | 0x4
|  | ASCC_PERIODS_6 | Measure 6 asynchronous clock periods | 0x5
|  | ASCC_PERIODS_7 | Measure 7 asynchronous clock periods | 0x6
|  | ASCC_PERIODS_8 | Measure 8 asynchronous clock periods | 0x7
|  | ASCC_PERIODS_9 | Measure 9 asynchronous clock periods | 0x8
|  | ASCC_PERIODS_10 | Measure 10 asynchronous clock periods | 0x9
|  | ASCC_PERIODS_11 | Measure 11 asynchronous clock periods | 0xA
|  | ASCC_PERIODS_12 | Measure 12 asynchronous clock periods | 0xB
|  | ASCC_PERIODS_13 | Measure 13 asynchronous clock periods | 0xC
|  | ASCC_PERIODS_14 | Measure 14 asynchronous clock periods | 0xD
|  | ASCC_PERIODS_15 | Measure 15 asynchronous clock periods | 0xE
|  | ASCC_PERIODS_16 | Measure 16 asynchronous clock periods | 0xF