### NVIC_ISPR1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
24 | RW | DMA3 | DMA3 interrupt set pending
23 | RW | DMA2 | DMA2 interrupt set pending
22 | RW | DMA1 | DMA1 interrupt set pending
21 | RW | DMA0 | DMA0 interrupt set pending
20 | RW | ACCESS_ERROR | ACCESS_ERROR interrupt set pending
19 | RW | FLASH0_ECC | FLASH0_ECC interrupt set pending
18 | RW | FLASH0_COPY | FLASH0_COPY interrupt set pending
17 | RW | RF_RXFIFO | RF_RXFIFO interrupt set pending
16 | RW | RF_TXFIFO | RF_TXFIFO interrupt set pending
15 | RW | RF_SYNC | RF_SYNC interrupt set pending
14 | RW | RF_IRQ_RECEIVED | RF_IRQ_RECEIVED interrupt set pending
13 | RW | RF_RXSTOP | RF_RXSTOP interrupt set pending
12 | RW | RF_TX | RF_TX interrupt set pending
11 | RW | TOF | TOF interrupt set pending
10 | RW | BLE_COEX_RX_TX | BLE_COEX_RX_TX interrupt set pending
9 | RW | BLE_COEX_IN_PROCESS | BLE_COEX_IN_PROCESS interrupt set pending
8 | RW | BLE_ERROR | BLE_ERROR interrupt set pending
7 | RW | BLE_FIFO | BLE_FIFO interrupt set pending
6 | RW | BLE_HSLOT | BLE_HSLOT interrupt set pending
5 | RW | BLE_SLP | BLE_SLP interrupt set pending
4 | RW | BLE_CRYPT | BLE_CRYPT interrupt set pending
3 | RW | BLE_TIMESTAMP_TGT2 | BLE_TIMESTAMP_TGT2 interrupt set pending
2 | RW | BLE_TIMESTAMP_TGT1 | BLE_TIMESTAMP_TGT1 interrupt set pending
1 | RW | BLE_FINETGT | BLE_FINETGT interrupt set pending
0 | RW | BLE_SW | BLE_SW interrupt set pending

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
24 | DMA3 | NVIC_DMA3_INT_SETPEND | Set the DMA3 interrupt pending | 0x1
23 | DMA2 | NVIC_DMA2_INT_SETPEND | Set the DMA2 interrupt pending | 0x1
22 | DMA1 | NVIC_DMA1_INT_SETPEND | Set the DMA1 interrupt pending | 0x1
21 | DMA0 | NVIC_DMA0_INT_SETPEND | Set the DMA0 interrupt pending | 0x1
20 | ACCESS_ERROR | NVIC_ACCESS_ERROR_INT_SETPEND | Set the ACCESS_ERROR interrupt pending | 0x1
19 | FLASH0_ECC | NVIC_FLASH0_ECC_INT_SETPEND | Set the FLASH0_ECC interrupt pending | 0x1
18 | FLASH0_COPY | NVIC_FLASH0_COPY_INT_SETPEND | Set the FLASH0_COPY interrupt pending | 0x1
17 | RF_RXFIFO | NVIC_RF_RXFIFO_INT_SETPEND | Set the RF_RXFIFO interrupt pending | 0x1
16 | RF_TXFIFO | NVIC_RF_TXFIFO_INT_SETPEND | Set the RF_TXFIFO interrupt pending | 0x1
15 | RF_SYNC | NVIC_RF_SYNC_INT_SETPEND | Set the RF_SYNC interrupt pending | 0x1
14 | RF_IRQ_RECEIVED | NVIC_RF_IRQ_RECEIVED_INT_SETPEND | Set the RF_IRQ_RECEIVED interrupt pending | 0x1
13 | RF_RXSTOP | NVIC_RF_RXSTOP_INT_SETPEND | Set the RF_RXSTOP interrupt pending | 0x1
12 | RF_TX | NVIC_RF_TX_INT_SETPEND | Set the RF_TX interrupt pending | 0x1
11 | TOF | NVIC_TOF_INT_SETPEND | Set the TOF interrupt pending | 0x1
10 | BLE_COEX_RX_TX | NVIC_BLE_COEX_RX_TX_INT_SETPEND | Set the BLE_COEX_RX_TX interrupt pending | 0x1
9 | BLE_COEX_IN_PROCESS | NVIC_BLE_COEX_IN_PROCESS_INT_SETPEND | Set the BLE_COEX_IN_PROCESS interrupt pending | 0x1
8 | BLE_ERROR | NVIC_BLE_ERROR_INT_SETPEND | Set the BLE_ERROR interrupt pending | 0x1
7 | BLE_FIFO | NVIC_BLE_FIFO_INT_SETPEND | Set the BLE_FIFO interrupt pending | 0x1
6 | BLE_HSLOT | NVIC_BLE_HSLOT_INT_SETPEND | Set the BLE_HSLOT interrupt pending | 0x1
5 | BLE_SLP | NVIC_BLE_SLP_INT_SETPEND | Set the BLE_SLP interrupt pending | 0x1
4 | BLE_CRYPT | NVIC_BLE_CRYPT_INT_SETPEND | Set the BLE_CRYPT interrupt pending | 0x1
3 | BLE_TIMESTAMP_TGT2 | NVIC_BLE_TIMESTAMP_TGT2_INT_SETPEND | Set the BLE_TIMESTAMP_TGT2 interrupt pending | 0x1
2 | BLE_TIMESTAMP_TGT1 | NVIC_BLE_TIMESTAMP_TGT1_INT_SETPEND | Set the BLE_TIMESTAMP_TGT1 interrupt pending | 0x1
1 | BLE_FINETGT | NVIC_BLE_FINETGT_INT_SETPEND | Set the BLE_FINETGT interrupt pending | 0x1
0 | BLE_SW | NVIC_BLE_SW_INT_SETPEND | Set the BLE_SW interrupt pending | 0x1