### ACS_TEMP_SENSOR_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
1 | RW | DUTY_TEMP_SENS | Duty cycling temperature sensor
0 | RW | ENABLE | Internal temperature sensor enable

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
1 | DUTY_TEMP_SENS | LSAD_TEMP_SENS_NORMAL | Normal mode: temperature sensor enable only controlled by TEMP_SENS_ENABLE | 0x0*
|  | LSAD_TEMP_SENS_DUTY | Duty cycling temperature sensor (enabled only during LSAD conversion) | 0x1
0 | ENABLE | TEMP_SENS_DISABLE | Disable the internal Temperature Sensor | 0x0*
|  | TEMP_SENS_ENABLE | Enable the internal Temperature Sensor | 0x1