### WATCHDOG_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
3:0 | RW | TIMEOUT_VALUE | Watchdog timeout period. Values 0xC to 0xF result in the same timeout period as the value 0xB.

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
3:0 | TIMEOUT_VALUE | WATCHDOG_TIMEOUT_2M048 | 2.048 ms | 0x0
|  | WATCHDOG_TIMEOUT_4M096 | 4.096 ms | 0x1
|  | WATCHDOG_TIMEOUT_8M2 | 8.192 ms | 0x2
|  | WATCHDOG_TIMEOUT_16M4 | 16.384 ms | 0x3
|  | WATCHDOG_TIMEOUT_32M8 | 32.768 ms | 0x4
|  | WATCHDOG_TIMEOUT_65M5 | 65.536 ms | 0x5
|  | WATCHDOG_TIMEOUT_131M1 | 131.072 ms | 0x6
|  | WATCHDOG_TIMEOUT_262M1 | 262.144 ms | 0x7
|  | WATCHDOG_TIMEOUT_524M3 | 524.3 ms | 0x8
|  | WATCHDOG_TIMEOUT_1048M6 | 1.048 sec | 0x9
|  | WATCHDOG_TIMEOUT_2097M1 | 2.097 sec | 0xA
|  | WATCHDOG_TIMEOUT_4194M3 | 4.194 sec | 0xB*