### BB_INTCNTL1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
30:28 | RW | CLKNINTSRMSK | CLKN/half-slot interrupt sub rating mask (valid range is [0:4])
27:24 | RW | CLKNINTSRVAL | CLKN/half-slot interrupt sub rating value
15 | RW | FIFOINTMSK | FIFO interrupt mask
6 | RW | TIMESTAMPTGT2INTMSK | Time stamp target timer 2 interrupt mask
5 | RW | TIMESTAMPTGT1INTMSK | Time stamp target timer 1 interrupt mask
4 | RW | FINETGTIMINTMSK | Fine target timer interrupt mask
3 | RW | SWINTMSK | SW triggered interrupt mask
2 | RW | CRYPTINTMSK | Encryption engine interrupt mask
1 | RW | SLPINTMSK | Sleep mode interrupt mask
0 | RW | CLKNINTMSK | CLKN/half slot interrupt mask

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
30:28 | CLKNINTSRMSK | CLKNINTSRMSK_0 |  | 0x0*
27:24 | CLKNINTSRVAL | CLKNINTSRVAL_0 |  | 0x0*
15 | FIFOINTMSK | FIFOINTMSK_0 | Interrupt not generated | 0x0
|  | FIFOINTMSK_1 | Interrupt generated | 0x1*
6 | TIMESTAMPTGT2INTMSK | TIMESTAMPTGT2INTMSK_0 | Interrupt not generated | 0x0*
|  | TIMESTAMPTGT2INTMSK_1 | Interrupt generated | 0x1
5 | TIMESTAMPTGT1INTMSK | TIMESTAMPTGT1INTMSK_0 | Interrupt not generated | 0x0*
|  | TIMESTAMPTGT1INTMSK_1 | Interrupt generated | 0x1
4 | FINETGTIMINTMSK | FINETGTIMINTMSK_0 | Interrupt not generated | 0x0*
|  | FINETGTIMINTMSK_1 | Interrupt generated | 0x1
3 | SWINTMSK | SWINTMSK_0 | Interrupt not generated | 0x0*
|  | SWINTMSK_1 | Interrupt generated | 0x1
2 | CRYPTINTMSK | CRYPTINTMSK_0 | Interrupt not generated | 0x0*
|  | CRYPTINTMSK_1 | Interrupt generated | 0x1
1 | SLPINTMSK | SLPINTMSK_0 | Interrupt not generated | 0x0
|  | SLPINTMSK_1 | Interrupt generated | 0x1*
0 | CLKNINTMSK | CLKNINTMSK_0 | Interrupt not generated | 0x0
|  | CLKNINTMSK_1 | Interrupt generated | 0x1*