### BB_DFCNTL0_2US

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | RXSAMPSTINST0_2US | Adjustement delay in half us of Rx I and Q sampling start instant for LE 1M PHY (with 2us sampling interval)
23:16 | RW | RXSWSTINST0_2US | Adjustement delay in half us of Rx switch start instant for LE 1M PHY (with 2us switching interval)
7:0 | RW | TXSWSTINST0_2US | Adjustement delay in half us of Tx switch start instant for LE 1M PHY (with 2us switching interval)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | RXSAMPSTINST0_2US | RXSAMPSTINST0_2US_0 |  | 0x0*
23:16 | RXSWSTINST0_2US | RXSWSTINST0_2US_0 |  | 0x0*
7:0 | TXSWSTINST0_2US | TXSWSTINST0_2US_0 |  | 0x0*