### BB_SLOTCLK

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | SAMP | Sample the CLKN counter value in SCLK register field
30 | RW | CLKN_UPD | Update CLKN counter
27:0 | RW | SCLK | Value of the 312.5us CLKN counter

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | SAMP | SAMP_0 | No action happens if it is written with 0 | 0x0*
|  | SAMP_1 | Sample the CLKN Counter value in SCLK register field | 0x1
30 | CLKN_UPD | CLKN_UPD_0 | No action happens if it is written with 0 | 0x0*
|  | CLKN_UPD_1 | Update CLKN counter | 0x1
27:0 | SCLK | SCLK_0 |  | 0x0*