### RF_AGC_ATT2

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:28 | RW | TIMINGS_3_T_DLL | Time needed by the DLL blocks to switch on
27:24 | RW | TIMINGS_3_T_PLL_TX | Time needed by the PLL blocks in Tx mode to switch on
23:20 | RW | TIMINGS_2_T_SUBBAND_TX | Time needed by the subband algorithm to calibrate in Tx mode
19:16 | RW | TIMINGS_2_T_TX_RF | Time needed by the RF blocks to switch on in Tx mode
14:12 | RW | TIMINGS_1_T_GRANULARITY_TX | Define the granularity of the timer in Tx mode
10:8 | RW | TIMINGS_1_T_GRANULARITY_RX | Define the granularity of the timer in Rx mode
1 | RW | AGC_ATT_2_AGC_ATT_1DB | Attenuation steps
0 | RW | AGC_ATT_2_AGC_ATT_AB_HI | AGC attenuation step 10/11 (MSB)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:28 | TIMINGS_3_T_DLL | TIMINGS_3_T_DLL_DEFAULT |  | 0x2*
27:24 | TIMINGS_3_T_PLL_TX | TIMINGS_3_T_PLL_TX_DEFAULT |  | 0x2*
23:20 | TIMINGS_2_T_SUBBAND_TX | TIMINGS_2_T_SUBBAND_TX_DEFAULT |  | 0xC*
19:16 | TIMINGS_2_T_TX_RF | TIMINGS_2_T_TX_RF_DEFAULT |  | 0x1*
14:12 | TIMINGS_1_T_GRANULARITY_TX | TIMINGS_1_T_GRANULARITY_TX_DEFAULT | The granularity is given by (2^(t_granularity-2)) x 1us | 0x3*
10:8 | TIMINGS_1_T_GRANULARITY_RX | TIMINGS_1_T_GRANULARITY_RX_DEFAULT | The granularity is given by (2^(t_granularity)) x 1us) | 0x5*
1 | AGC_ATT_2_AGC_ATT_1DB | AGC_ATT_2_AGC_ATT_1DB_DISABLE | Attenuation is not specified by 1dB steps from 4dB to 11dB | 0x0*
|  | AGC_ATT_2_AGC_ATT_1DB_ENABLE | Attenuation is specified by 1dB steps from 4dB to 11dB | 0x1
0 | AGC_ATT_2_AGC_ATT_AB_HI | AGC_ATT_2_AGC_ATT_AB_HI_DISABLE | AGC_ATT_2_AGC_ATT_AB MSB is 0 | 0x0
|  | AGC_ATT_2_AGC_ATT_AB_HI_ENABLE | AGC_ATT_2_AGC_ATT_AB MSB is 1 | 0x1*