### RF_PADS_47

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
28:24 | RW | PAD_CONF_2_PAD_7_CONF | Configuration of GPIO pad 7
20:16 | RW | PAD_CONF_2_PAD_6_CONF | Configuration of GPIO pad 6
12:8 | RW | PAD_CONF_2_PAD_5_CONF | Configuration of GPIO pad 5
4:0 | RW | PAD_CONF_2_PAD_4_CONF | Configuration of GPIO pad 4

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
28:24 | PAD_CONF_2_PAD_7_CONF | PAD_CONF_2_PAD_7_OFF |  | 0x0*
|  | PAD_CONF_2_PAD_7_TEST_MODE |  | 0xF
20:16 | PAD_CONF_2_PAD_6_CONF | PAD_CONF_2_PAD_6_OFF |  | 0x0*
|  | PAD_CONF_2_PAD_6_TEST_MODE |  | 0xF
12:8 | PAD_CONF_2_PAD_5_CONF | PAD_CONF_2_PAD_5_OFF |  | 0x0*
|  | PAD_CONF_2_PAD_5_TEST_MODE |  | 0xF
4:0 | PAD_CONF_2_PAD_4_CONF | PAD_CONF_2_PAD_4_OFF |  | 0x0*
|  | PAD_CONF_2_PAD_4_TEST_MODE |  | 0xF