### ACS_PWR_MODES_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:0 | W | POWER_MODE | 32-bit key to enter STANDBY or SLEEP mode. This register must be written using a 32-bit access.

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:0 | POWER_MODE | PWR_RUN_MODE | Keep the system in normal RUN mode | 0x0*
|  | PWR_STANDBY_MODE | Enter STANDBY mode | 0x9B1D79A0
|  | PWR_SLEEP_MODE | Enter SLEEP mode | 0xE0045650