### TOF_LINK_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
16:12 | RW | LINK_FORMAT | Configure the link format for BLE link filtering
8:4 | RW | LINK_LABEL | Configure the link label for BLE link filtering
0 | RW | LINK_FILTER_EN | Enable the BLE link filtering based on link label and format

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
16:12 | LINK_FORMAT | TOF_LINK_FORMAT | Format of the BLE link to filter in the radio interrupts | 0x0*
8:4 | LINK_LABEL | TOF_LINK_LABEL | Label of the BLE link to filter in the radio interrupts | 0x0*
0 | LINK_FILTER_EN | TOF_LINK_FILTER_DISABLE | Disable external start trigger | 0x0*
|  | TOF_LINK_FILTER_ENABLE | Select TX radio interrupt to start the Time of flight timer | 0x1