### RF_BLE_LR

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
30:24 | RW | BLR_SYNC_THRESHOLD_BLE_SYNC_THR | Threshold for the BLR sync word detector
19:16 | RW | BLR_PREAMBLE_BLE_PRE_THR | Threshold for the BLR preamble detector
15 | RW | BLE_LONG_RANGE_BLR_PUT_RI_FIFO | During the reception the RI (rate indicator) is put into the Rx FIFO (banked)
14 | RW | BLE_LONG_RANGE_BLR500_NO_ROUGH | Rough recovery is stopped during the 500kbps payloads of BLR packets (banked)
13 | RW | BLE_LONG_RANGE_BLR_LIN_FILTER | Matched filter (banked)
12 | RW | BLE_LONG_RANGE_EN_BLR_FLUSH | Viterbi path 0 flushing at the end of the packet (banked)
11 | RW | BLE_LONG_RANGE_BLR_USE_EXT_LEN | BLR_PKT_LEN for flushing out the Viterbi (banked)
10 | RW | BLE_LONG_RANGE_DISABLE_BLR_TX | Long Range feature in Tx mode (banked)
9 | RW | BLE_LONG_RANGE_BLR_500_N125 | Data rate selection (banked)
8 | RW | BLE_LONG_RANGE_EN_BLR | BLE long range mode (banked)
4 | RW | HW_TRIGGER_HW_TRIG_GPIO | HW trigger is mapped on the GPIO instead of the Tx_on signal 0x0
3 | RW | HW_TRIGGER_HW_TRIG_SUBBAND | Activate the sub-band selection during the Tx activation
2 | RW | HW_TRIGGER_HW_TRIG_TX_NRX | Activate the Tx mode
1 | RW | HW_TRIGGER_HW_TRIG_LOW | Set the trigger polarity
0 | RW | HW_TRIGGER_HW_TRIG_ACTIVE | Enable HW trigger

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
30:24 | BLR_SYNC_THRESHOLD_BLE_SYNC_THR | BLR_SYNC_THRESHOLD_BLE_SYNC_THR_DEFAULT | Unsigned value smaller than 64 | 0x38*
19:16 | BLR_PREAMBLE_BLE_PRE_THR | BLR_PREAMBLE_BLE_PRE_THR_DEFAULT | Unsigned value | 0x1*
15 | BLE_LONG_RANGE_BLR_PUT_RI_FIFO | BLE_LONG_RANGE_BLR_PUT_RI_FIFO_DISABLE | Do not put RI in the RX FIFO | 0x0
|  | BLE_LONG_RANGE_BLR_PUT_RI_FIFO_ENABLE | Put RI in the RX FIFO | 0x1*
14 | BLE_LONG_RANGE_BLR500_NO_ROUGH | BLE_LONG_RANGE_BLR500_NO_ROUGH_NO_STOP | Rough recovery is not stopped | 0x0
|  | BLE_LONG_RANGE_BLR500_NO_ROUGH_STOP | Rough recovery is stopped | 0x1*
13 | BLE_LONG_RANGE_BLR_LIN_FILTER | BLE_LONG_RANGE_BLR_LIN_FILTER_DISABLE | The matched filter is not linear in BLR mode | 0x0
|  | BLE_LONG_RANGE_BLR_LIN_FILTER_ENABLE | The matched filter is linear in BLR mode | 0x1*
12 | BLE_LONG_RANGE_EN_BLR_FLUSH | BLE_LONG_RANGE_EN_BLR_FLUSH_DISABLE | The Viterbi path 0 is not flushed at 2Mbps | 0x0
|  | BLE_LONG_RANGE_EN_BLR_FLUSH_ENABLE | The Viterbi path 0 is flushed at 2Mbps | 0x1*
11 | BLE_LONG_RANGE_BLR_USE_EXT_LEN | BLE_LONG_RANGE_BLR_USE_EXT_LEN_NOT_USED | The value in BLR_PKT_LEN will not be used for the flush out of the Viterbi at the end of the packet | 0x0*
|  | BLE_LONG_RANGE_BLR_USE_EXT_LEN_USED | The value in BLR_PKT_LEN will be used for the flush out of the Viterbi at the end of the packet | 0x1
10 | BLE_LONG_RANGE_DISABLE_BLR_TX | BLE_LONG_RANGE_DISABLE_BLR_TX_ENABLE | Long Range feature is enabled in Tx mode | 0x0*
|  | BLE_LONG_RANGE_DISABLE_BLR_TX_DISABLE | Long Range feature is disabled in Tx mode | 0x1
9 | BLE_LONG_RANGE_BLR_500_N125 | BLE_LONG_RANGE_BLR_500_N125_125 | 125 kbps mode is used | 0x0*
|  | BLE_LONG_RANGE_BLR_500_N125_500 | 500 kbps mode is used | 0x1
8 | BLE_LONG_RANGE_EN_BLR | BLE_LONG_RANGE_EN_BLR_DISABLE | Disable the BLE long range mode | 0x0*
|  | BLE_LONG_RANGE_EN_BLR_ENABLE | Enable the BLE long range mode | 0x1
4 | HW_TRIGGER_HW_TRIG_GPIO | HW_TRIGGER_HW_TRIG_GPIO_TX_ON | HW trigger mapped on TX_ON | 0x0*
|  | HW_TRIGGER_HW_TRIG_GPIO | HW trigger mapped on GPIO | 0x1
3 | HW_TRIGGER_HW_TRIG_SUBBAND | HW_TRIGGER_HW_TRIG_SUBBAND_NOT_ACTIVE | HW trigger does not active sub-band selection | 0x0*
|  | HW_TRIGGER_HW_TRIG_SUBBAND_ACTIVE | HW trigger actives sub-band selection | 0x1
2 | HW_TRIGGER_HW_TRIG_TX_NRX | HW_TRIGGER_HW_TRIG_TX_NRX_RX | HW trigger actives RX mode | 0x0*
|  | HW_TRIGGER_HW_TRIG_TX_NRX_TX | HW trigger actives TX mode | 0x1
1 | HW_TRIGGER_HW_TRIG_LOW | HW_TRIGGER_HW_TRIG_LOW_LOW | HW trigger active low | 0x0*
|  | HW_TRIGGER_HW_TRIG_LOW_HIGH | HW trigger active high | 0x1
0 | HW_TRIGGER_HW_TRIG_ACTIVE | HW_TRIGGER_HW_TRIG_ACTIVE_DISABLE | Disable HW trigger | 0x0*
|  | HW_TRIGGER_HW_TRIG_ACTIVE_ENABLE | Enable HW trigger | 0x1