### FPE_FPCCR

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | ASPEN | When this bit is set to 1, execution of a floating-point instruction sets the CONTROL.FPCA bit to 1
30 | RW | LSPEN | Enable lazy contect save of FP state
29 | RW | LSPENS | This bit controls whether the LSPEN bit is writable from the Non-secure state
28 | RW | CLRONRET | Clear floating point caller saved register on exception return
27 | RW | CLRONRETS | CLRONRET secure only
26 | RW | TS | Threat FP registers as Secure enable
10 | RW | UFRDY | Indicates whether the software executing when the processor allocated the floating-point stack frame was able to set the Usage Fault exeption to pending.
9 | RW | SPLIMVIOL | This bit is banked between the Security states and indicates whether the floating-point context violates the stack pointer limit that was active when lazy state preservation was activated.
8 | RW | MONRDY | Indicates whether the software executing when the processor allocated the floating-point stack frame was able to set the debug monitor execption to pending.
7 | RW | SFRDY | Indicates whether the software executing when the processor allocated the floating-point stack frame was able to set the secure fault exception to pending.
6 | RW | BRDY | Indicates whether the software executing when the processor allocated the floating-point stack frame was able to set the bus fault exception to pending.
5 | RW | MMRDY | Indicates whether the software executing when the processor allocated the floating-point stack frame was able to set the Mem Manage exception to pending.
4 | RW | HFRDY | Indicates whether the software executing when the processor allocated the floating-point stack frame was able to set the Hard fault exception to pending.
3 | RW | THREAD | Indicates the processor mode when it allocated the floating-point stack frame.
2 | RW | S | Security status of the floating-point context
1 | RW | USER | Indicates the privilege level of the software executing when the processor allocated the floating-point stack frame
0 | RW | LSPACT | Indicates whether lazy preservation of the floating-point state is active.