### ACS_SLEEP_MODE_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
2 | RW | BG_ENABLE | Keep Band-gap enabled during sleep
1 | RW | VCC_ENABLE | Keep VCC low power enabled during sleep
0 | RW | VDDCP_ENABLE | Keep VDDCP charge pump enabled during sleep

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
2 | BG_ENABLE | BG_DISABLE_IN_SLEEP | Band-gap disabled in sleep | 0x0*
|  | BG_ENABLE_IN_SLEEP | Band-gap enabled in sleep | 0x1
1 | VCC_ENABLE | VCC_DISABLE_IN_SLEEP | VCC disabled in sleep | 0x0*
|  | VCC_ENABLE_IN_SLEEP | VCC enabled in sleep | 0x1
0 | VDDCP_ENABLE | VDDCP_DISABLE_IN_SLEEP | Charge pump disabled in sleep | 0x0*
|  | VDDCP_ENABLE_IN_SLEEP | Charge pump enabled in sleep | 0x1