### BB_RADIOCNTL3

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:30 | RW | RXRATE3CFG | Rate out programmable value in Rx when CS-RXRATE is set to 0x3 (i.e 500kbps Long range)
29:28 | RW | RXRATE2CFG | Rate out programmable value in Rx when CS-RXRATE is set to 0x2 (i.e 125kbps Long range)
27:26 | RW | RXRATE1CFG | Rate out programmable value in Rx when CS-RXRATE is set to 0x1 (i.e 2Mbps)
25:24 | RW | RXRATE0CFG | Rate out programmable value in Rx when CS-RXRATE is set to 0x0 (i.e 1Mbps)
22:20 | RW | GETRSSIDELAY | Delay to read RSSI after an RSSI read request
18 | RW | RXSYNC_ROUTING | Access address detection information routing
17:16 | RW | RXVALID_BEH | Define radio_in[3] expected behavior
15:14 | RW | TXRATE3CFG | Rate out programmable value in Tx when CS-TX/AUX-RATE is set to 0x3 (i.e 500kbps Long range)
13:12 | RW | TXRATE2CFG | Rate out programmable value in Tx when CS-TX/AUX-RATE is set to 0x2 (i.e 125kbps Long range)
11:10 | RW | TXRATE1CFG | Rate out programmable value in Tx when CS-TX/AUX-RATE is set to 0x1 (i.e 2Mbps)
9:8 | RW | TXRATE0CFG | Rate out programmable value in Tx when CS-TX/AUX-RATE is set to 0x0 (i.e 1Mbps)
1:0 | RW | TXVALID_BEH | Define radio_out [3] expected behavior

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:30 | RXRATE3CFG | RXRATE3CFG_3 |  | 0x3*
29:28 | RXRATE2CFG | RXRATE3CFG_2 |  | 0x2*
27:26 | RXRATE1CFG | RXRATE3CFG_1 |  | 0x1*
25:24 | RXRATE0CFG | RXRATE3CFG_0 |  | 0x0*
22:20 | GETRSSIDELAY | GETRSSIDELAY_4 |  | 0x4*
18 | RXSYNC_ROUTING | RXSYNC_ROUTING_0 | Uses radio_in[16] (i.e sync_p) | 0x0*
|  | RXSYNC_ROUTING_1 | Uses first radio_in[3] edge (Rx Valid) | 0x1
17:16 | RXVALID_BEH | RXVALID_BEH_0 | Rx data aligned on radio_in[3] rising edges | 0x0*
|  | RXVALID_BEH_1 | Rx data aligned on radio_in[3] falling edges | 0x1
|  | RXVALID_BEH_2 | Rx data aligned on radio_in[3] edges (toggle mode) | 0x2
|  | RXVALID_BEH_3 | NA | 0x3
15:14 | TXRATE3CFG | TXRATE3CFG_3 |  | 0x3*
13:12 | TXRATE2CFG | TXRATE3CFG_2 |  | 0x2*
11:10 | TXRATE1CFG | TXRATE3CFG_1 |  | 0x1*
9:8 | TXRATE0CFG | TXRATE3CFG_0 |  | 0x0*
1:0 | TXVALID_BEH | TXVALID_BEH_0 | Tx data aligned on radio_out[3] rising edges | 0x0*
|  | TXVALID_BEH_1 | Tx data aligned on radio_out[3] falling edges | 0x1
|  | TXVALID_BEH_2 | Tx data aligned on radio_out[3] edges (toggle mode) | 0x2
|  | TXVALID_BEH_3 | NA | 0x3