### NVIC_ICER0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | ASCC_PHASE | ASCC_PHASE interrupt clear enable
30 | RW | ASCC_PERIOD | ASCC_PERIOD interrupt clear enable
29 | RW | CC312 | CC312 interrupt clear enable
28 | RW | FPU | FPU interrupt clear enable
27 | RW | LIN0 | LIN0 interrupt clear enable
26 | RW | PCM0_ERROR | PCM0_ERROR interrupt clear enable
25 | RW | PCM0_RX_TX | PCM0_RX_TX interrupt clear enable
24 | RW | UART0_ERROR | UART0_ERROR interrupt clear enable
23 | RW | UART0_TX | UART0_TX interrupt clear enable
22 | RW | UART0_RX | UART0_RX interrupt clear enable
21 | RW | I2C1 | I2C1 interrupt clear enable
20 | RW | I2C0 | I2C0 interrupt clear enable
19 | RW | SPI1_COM | SPI1_COM interrupt clear enable
18 | RW | SPI1_TX | SPI1_TX interrupt clear enable
17 | RW | SPI1_RX | SPI1_RX interrupt clear enable
16 | RW | SPI0_COM | SPI0_COM interrupt clear enable
15 | RW | SPI0_TX | SPI0_TX interrupt clear enable
14 | RW | SPI0_RX | SPI0_RX interrupt clear enable
13 | RW | WATCHDOG | WATCHDOG interrupt clear enable
12 | RW | GPIO3 | GPIO3 interrupt clear enable
11 | RW | GPIO2 | GPIO2 interrupt clear enable
10 | RW | GPIO1 | GPIO1 interrupt clear enable
9 | RW | GPIO0 | GPIO0 interrupt clear enable
8 | RW | FIFO | FIFO interrupt clear enable
7 | RW | TIMER3 | TIMER3 interrupt clear enable
6 | RW | TIMER2 | TIMER2 interrupt clear enable
5 | RW | TIMER1 | TIMER1 interrupt clear enable
4 | RW | TIMER0 | TIMER0 interrupt clear enable
3 | RW | LSAD_MONITOR | LSAD_MONITOR interrupt clear enable
2 | RW | RTC_CLOCK | RTC_CLOCK interrupt clear enable
1 | RW | RTC_ALARM | RTC_ALARM interrupt clear enable
0 | RW | WAKEUP | WAKEUP interrupt clear enable

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | ASCC_PHASE | NVIC_ASCC_PHASE_INT_DISABLE | Disable the ASCC_PHASE interrupt | 0x1
30 | ASCC_PERIOD | NVIC_ASCC_PERIOD_INT_DISABLE | Disable the ASCC_PERIOD interrupt | 0x1
29 | CC312 | NVIC_CC312_INT_DISABLE | Disable the CC312 interrupt | 0x1
28 | FPU | NVIC_FPU_INT_DISABLE | Disable the FPU interrupt | 0x1
27 | LIN0 | NVIC_LIN0_INT_DISABLE | Disable the LIN0 interrupt | 0x1
26 | PCM0_ERROR | NVIC_PCM0_ERROR_INT_DISABLE | Disable the PCM0_ERROR interrupt | 0x1
25 | PCM0_RX_TX | NVIC_PCM0_RX_TX_INT_DISABLE | Disable the PCM0_RX_TX interrupt | 0x1
24 | UART0_ERROR | NVIC_UART0_ERROR_INT_DISABLE | Disable the UART0_ERROR interrupt | 0x1
23 | UART0_TX | NVIC_UART0_TX_INT_DISABLE | Disable the UART0_TX interrupt | 0x1
22 | UART0_RX | NVIC_UART0_RX_INT_DISABLE | Disable the UART0_RX interrupt | 0x1
21 | I2C1 | NVIC_I2C1_INT_DISABLE | Disable the I2C1 interrupt | 0x1
20 | I2C0 | NVIC_I2C0_INT_DISABLE | Disable the I2C0 interrupt | 0x1
19 | SPI1_COM | NVIC_SPI1_COM_INT_DISABLE | Disable the SPI1_COM interrupt | 0x1
18 | SPI1_TX | NVIC_SPI1_TX_INT_DISABLE | Disable the SPI1_TX interrupt | 0x1
17 | SPI1_RX | NVIC_SPI1_RX_INT_DISABLE | Disable the SPI1_RX interrupt | 0x1
16 | SPI0_COM | NVIC_SPI0_COM_INT_DISABLE | Disable the SPI0_COM interrupt | 0x1
15 | SPI0_TX | NVIC_SPI0_TX_INT_DISABLE | Disable the SPI0_TX interrupt | 0x1
14 | SPI0_RX | NVIC_SPI0_RX_INT_DISABLE | Disable the SPI0_RX interrupt | 0x1
13 | WATCHDOG | NVIC_WATCHDOG_INT_DISABLE | Disable the WATCHDOG interrupt | 0x1
12 | GPIO3 | NVIC_GPIO3_INT_DISABLE | Disable the GPIO3 interrupt | 0x1
11 | GPIO2 | NVIC_GPIO2_INT_DISABLE | Disable the GPIO2 interrupt | 0x1
10 | GPIO1 | NVIC_GPIO1_INT_DISABLE | Disable the GPIO1 interrupt | 0x1
9 | GPIO0 | NVIC_GPIO0_INT_DISABLE | Disable the GPIO0 interrupt | 0x1
8 | FIFO | NVIC_FIFO_INT_DISABLE | Disable the FIFO interrupt | 0x1
7 | TIMER3 | NVIC_TIMER3_INT_DISABLE | Disable the TIMER3 interrupt | 0x1
6 | TIMER2 | NVIC_TIMER2_INT_DISABLE | Disable the TIMER2 interrupt | 0x1
5 | TIMER1 | NVIC_TIMER1_INT_DISABLE | Disable the TIMER1 interrupt | 0x1
4 | TIMER0 | NVIC_TIMER0_INT_DISABLE | Disable the TIMER0 interrupt | 0x1
3 | LSAD_MONITOR | NVIC_LSAD_MONITOR_INT_DISABLE | Disable the LSAD_MONITOR interrupt | 0x1
2 | RTC_CLOCK | NVIC_RTC_CLOCK_INT_DISABLE | Disable the RTC_CLOCK interrupt | 0x1
1 | RTC_ALARM | NVIC_RTC_ALARM_INT_DISABLE | Disable the RTC_ALARM interrupt | 0x1
0 | WAKEUP | NVIC_WAKEUP_INT_DISABLE | Disable the WAKEUP interrupt | 0x1