### RF_REG01

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | TAU_PHASE_RECOV_TAU_PHASE_RECOV | Time constant of the fine carrier recovery block (banked)
23:16 | RW | TAU_ROUGH_RECOV_TAU_ROUGH_RECOV | Time constant of the rough carrier recovery block (banked)
15 | RW | CARRIER_RECOVERY_EN_CORRECT_CFREQ_AFC | Automatic AFC correction (banked)
14 | RW | CARRIER_RECOVERY_CORRECT_CFREQ_IF_NEG | IF correction (banked)
13 | RW | CARRIER_RECOVERY_EN_CORRECT_CFREQ_IF | Automatic IF correction (banked)
12 | RW | CARRIER_RECOVERY_AFC_NEG | AFC correction (banked)
11 | RW | CARRIER_RECOVERY_STARTER_MODE | Starter mode (banked)
10 | RW | CARRIER_RECOVERY_EN_AFC | Automatic frequency control (banked)
9 | RW | CARRIER_RECOVERY_EN_FINE_RECOV | Fine carrier recovery (banked)
8 | RW | CARRIER_RECOVERY_EN_ROUGH_RECOV | Rough carrier recovery (banked)
6 | RW | MOD_TX_PULSE_NSYM | Tx pulse shape function
5 | RW | MOD_TX_EN_INTERP | Tx CIC interpolator
4:0 | RW | MOD_TX_CK_TX_M | Unsigned value determining the Tx CIC interpolator frequency

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | TAU_PHASE_RECOV_TAU_PHASE_RECOV | TAU_PHASE_RECOV_TAU_PHASE_RECOV_DEFAULT |  | 0x14*
23:16 | TAU_ROUGH_RECOV_TAU_ROUGH_RECOV | TAU_ROUGH_RECOV_TAU_ROUGH_RECOV_DEFAULT |  | 0xB*
15 | CARRIER_RECOVERY_EN_CORRECT_CFREQ_AFC | CARRIER_RECOVERY_EN_CORRECT_CFREQ_AFC_DISABLE | Disable the automatic AFC correction | 0x0*
|  | CARRIER_RECOVERY_EN_CORRECT_CFREQ_AFC_ENABLE | Enable the automatic AFC correction | 0x1
14 | CARRIER_RECOVERY_CORRECT_CFREQ_IF_NEG | CARRIER_RECOVERY_CORRECT_CFREQ_IF_NEG_POS | Positive IF correction | 0x0*
|  | CARRIER_RECOVERY_CORRECT_CFREQ_IF_NEG_NEG | Negative IF correction | 0x1
13 | CARRIER_RECOVERY_EN_CORRECT_CFREQ_IF | CARRIER_RECOVERY_EN_CORRECT_CFREQ_IF_DISABLE | Disable the automatic IF correction | 0x0
|  | CARRIER_RECOVERY_EN_CORRECT_CFREQ_IF_ENABLE | Enable the automatic IF correction | 0x1*
12 | CARRIER_RECOVERY_AFC_NEG | CARRIER_RECOVERY_AFC_NEG_POS | Positive AFC correction | 0x0*
|  | CARRIER_RECOVERY_AFC_NEG_NEG | Negative AFC correction | 0x1
11 | CARRIER_RECOVERY_STARTER_MODE | CARRIER_RECOVERY_STARTER_MODE_DISABLE | Disable the starter mode | 0x0*
|  | CARRIER_RECOVERY_STARTER_MODE_ENABLE | Enable the starter mode (32x faster carrier recovery) | 0x1
10 | CARRIER_RECOVERY_EN_AFC | CARRIER_RECOVERY_EN_AFC_DISABLE | Disable the Automatic Frequency Control | 0x0*
|  | CARRIER_RECOVERY_EN_AFC_ENABLE | Enable the Automatic Frequency Control | 0x1
9 | CARRIER_RECOVERY_EN_FINE_RECOV | CARRIER_RECOVERY_EN_FINE_RECOV_DISABLE | Disable the fine carrier recovery | 0x0
|  | CARRIER_RECOVERY_EN_FINE_RECOV_ENABLE | Enable the fine carrier recovery | 0x1*
8 | CARRIER_RECOVERY_EN_ROUGH_RECOV | CARRIER_RECOVERY_EN_ROUGH_RECOV_DISABLE | Disable the rough carrier recovery | 0x0*
|  | CARRIER_RECOVERY_EN_ROUGH_RECOV_ENABLE | Enable the rough carrier recovery | 0x1
6 | MOD_TX_PULSE_NSYM | MOD_TX_PULSE_NSYM_EVEN | Tx pulse shape is an even function | 0x0*
|  | MOD_TX_PULSE_NSYM_ODD | Tx pulse shape is an odd function | 0x1
5 | MOD_TX_EN_INTERP | MOD_TX_EN_INTERP_DISABLE | Disable the Tx CIC interpolator | 0x0*
|  | MOD_TX_EN_INTERP_ENABLE | Enable the Tx CIC interpolator | 0x1
4:0 | MOD_TX_CK_TX_M | MOD_TX_CK_TX_M_DEFAULT | The formula is similar to the evaluation of the oversampling frequency | 0x0*