### GPIO_SRC_BB_RX

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
20:16 | RW | SYNC_P | Baseband controller interface SYNC_P input selection
12:8 | RW | CLK | Baseband controller RX clock input selection
4:0 | RW | DATA | Baseband controller RX data input selection

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
20:16 | SYNC_P | BB_RX_SYNC_P_SRC_GPIO_0 | Select GPIO[0] as source | 0x0
|  | BB_RX_SYNC_P_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | BB_RX_SYNC_P_SRC_GPIO_2 | Select GPIO[5] as source | 0x2
|  | BB_RX_SYNC_P_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | BB_RX_SYNC_P_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | BB_RX_SYNC_P_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | BB_RX_SYNC_P_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | BB_RX_SYNC_P_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | BB_RX_SYNC_P_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | BB_RX_SYNC_P_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | BB_RX_SYNC_P_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | BB_RX_SYNC_P_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | BB_RX_SYNC_P_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | BB_RX_SYNC_P_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | BB_RX_SYNC_P_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | BB_RX_SYNC_P_SRC_GPIO_15 | Select GPIO[15] as source | 0xF
|  | BB_RX_SYNC_P_SRC_CONST_LOW | Select constant low as source | 0x10
|  | BB_RX_SYNC_P_SRC_CONST_HIGH | Select constant high as source | 0x11
|  | BB_RX_SYNC_P_SRC_RF_GPIO2 | Select RF front-end GPIO2 output (RX_SYNC_P) as source | 0x12*
12:8 | CLK | BB_RX_CLK_SRC_GPIO_0 | Select GPIO[0] as source | 0x0
|  | BB_RX_CLK_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | BB_RX_CLK_SRC_GPIO_2 | Select GPIO[2] as source | 0x2
|  | BB_RX_CLK_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | BB_RX_CLK_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | BB_RX_CLK_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | BB_RX_CLK_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | BB_RX_CLK_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | BB_RX_CLK_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | BB_RX_CLK_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | BB_RX_CLK_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | BB_RX_CLK_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | BB_RX_CLK_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | BB_RX_CLK_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | BB_RX_CLK_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | BB_RX_CLK_SRC_GPIO_15 | Select GPIO[15] as source | 0xF
|  | BB_RX_CLK_SRC_CONST_LOW | Select constant low as source | 0x10
|  | BB_RX_CLK_SRC_CONST_HIGH | Select constant high as source | 0x11
|  | BB_RX_CLK_SRC_RF_GPIO1 | Select RF front-end GPIO1 output (RX_CLK) as source | 0x12*
4:0 | DATA | BB_RX_DATA_SRC_GPIO_0 | Select GPIO[0] as source | 0x0
|  | BB_RX_DATA_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | BB_RX_DATA_SRC_GPIO_2 | Select GPIO[2] as source | 0x2
|  | BB_RX_DATA_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | BB_RX_DATA_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | BB_RX_DATA_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | BB_RX_DATA_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | BB_RX_DATA_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | BB_RX_DATA_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | BB_RX_DATA_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | BB_RX_DATA_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | BB_RX_DATA_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | BB_RX_DATA_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | BB_RX_DATA_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | BB_RX_DATA_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | BB_RX_DATA_SRC_GPIO_15 | Select GPIO[15] as source | 0xF
|  | BB_RX_DATA_SRC_CONST_LOW | Select constant low as source | 0x10
|  | BB_RX_DATA_SRC_CONST_HIGH | Select constant high as source | 0x11
|  | BB_RX_DATA_SRC_RF_GPIO0 | Select RF front-end GPIO0 output (RX_DATA) as source | 0x12*