### FLASH_MAIN_MASK

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
11 | R | DATA_A_35K_TO_40K_W_MASK | Authorize the access to the Flash MAIN Data array from 35K to 40K word block through the FLASH_IF registers.
10 | R | DATA_A_30K_TO_35K_W_MASK | Authorize the access to the Flash MAIN Data array from 30K to 35K word block through the FLASH_IF registers.
9 | R | DATA_A_25K_TO_30K_W_MASK | Authorize the access to the Flash MAIN Data array from 25K to 30K word block through the FLASH_IF registers.
8 | R | DATA_A_20K_TO_25K_W_MASK | Authorize the access to the Flash MAIN Data array from 20K to 25K word block through the FLASH_IF registers.
7 | R | DATA_A_15K_TO_20K_W_MASK | Authorize the access to the Flash MAIN Data array from 15K to 20K word block through the FLASH_IF registers.
6 | R | DATA_A_10K_TO_15K_W_MASK | Authorize the access to the Flash MAIN Data array from 10K to 15K word block through the FLASH_IF registers.
5 | R | DATA_A_5K_TO_10K_W_MASK | Authorize the access to the Flash MAIN Data array from 5K to 10K word block through the FLASH_IF registers.
4 | R | DATA_A_0K_TO_5K_W_MASK | Authorize the access to the Flash MAIN Data array from 0 to 5K word block through the FLASH_IF registers.
3 | R | CODE_A_66K_TO_88K_W_MASK | Authorize the access to the Flash MAIN Code array from 66K to 88K word block through the FLASH_IF registers.
2 | R | CODE_A_44K_TO_66K_W_MASK | Authorize the access to the Flash MAIN Code array from 44K to 66K word block through the FLASH_IF registers.
1 | R | CODE_A_22K_TO_44K_W_MASK | Authorize the access to the Flash MAIN Code array from 22K to 44K word block through the FLASH_IF registers.
0 | R | CODE_A_0K_TO_22K_W_MASK | Authorize the access to the Flash MAIN Code array from 0 to 22K word block through the FLASH_IF registers.

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
11 | DATA_A_35K_TO_40K_W_MASK | DATA_A_35K_TO_40K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Data array is not accessible. | 0x0
|  | DATA_A_35K_TO_40K_W_ACCESSIBLE | The part K to K of the Flash MAIN Data array is accessible. | 0x1*
10 | DATA_A_30K_TO_35K_W_MASK | DATA_A_30K_TO_35K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Data array is not accessible. | 0x0
|  | DATA_A_30K_TO_35K_W_ACCESSIBLE | The part K to K of the Flash MAIN Data array is accessible. | 0x1*
9 | DATA_A_25K_TO_30K_W_MASK | DATA_A_25K_TO_30K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Data array is not accessible. | 0x0
|  | DATA_A_25K_TO_30K_W_ACCESSIBLE | The part K to K of the Flash MAIN Data array is accessible. | 0x1*
8 | DATA_A_20K_TO_25K_W_MASK | DATA_A_20K_TO_25K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Data array is not accessible. | 0x0
|  | DATA_A_20K_TO_25K_W_ACCESSIBLE | The part K to K of the Flash MAIN Data array is accessible. | 0x1*
7 | DATA_A_15K_TO_20K_W_MASK | DATA_A_15K_TO_20K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Data array is not accessible. | 0x0
|  | DATA_A_15K_TO_20K_W_ACCESSIBLE | The part K to K of the Flash MAIN Data array is accessible. | 0x1*
6 | DATA_A_10K_TO_15K_W_MASK | DATA_A_10K_TO_15K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Data array is not accessible. | 0x0
|  | DATA_A_10K_TO_15K_W_ACCESSIBLE | The part K to K of the Flash MAIN Data array is accessible. | 0x1*
5 | DATA_A_5K_TO_10K_W_MASK | DATA_A_5K_TO_10K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Data array is not accessible. | 0x0
|  | DATA_A_5K_TO_10K_W_ACCESSIBLE | The part K to K of the Flash MAIN Data array is accessible. | 0x1*
4 | DATA_A_0K_TO_5K_W_MASK | DATA_A_0K_TO_5K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Data array is not accessible. | 0x0
|  | DATA_A_0K_TO_5K_W_ACCESSIBLE | The part K to K of the Flash MAIN Data array is accessible. | 0x1*
3 | CODE_A_66K_TO_88K_W_MASK | CODE_A_66K_TO_88K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Code array is not accessible. | 0x0
|  | CODE_A_66K_TO_88K_W_ACCESSIBLE | The part K to K of the Flash MAIN Code array is accessible. | 0x1*
2 | CODE_A_44K_TO_66K_W_MASK | CODE_A_44K_TO_66K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Code array is not accessible. | 0x0
|  | CODE_A_44K_TO_66K_W_ACCESSIBLE | The part K to K of the Flash MAIN Code array is accessible. | 0x1*
1 | CODE_A_22K_TO_44K_W_MASK | CODE_A_22K_TO_44K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Code array is not accessible. | 0x0
|  | CODE_A_22K_TO_44K_W_ACCESSIBLE | The part K to K of the Flash MAIN Code array is accessible. | 0x1*
0 | CODE_A_0K_TO_22K_W_MASK | CODE_A_0K_TO_22K_W_NOT_ACCESSIBLE | The part K to K of the Flash MAIN Code array is not accessible. | 0x0
|  | CODE_A_0K_TO_22K_W_ACCESSIBLE | The part K to K of the Flash MAIN Code array is accessible. | 0x1*