### RF_BIAS_3_6

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:28 | RW | BIAS_6_IQ_BB_0 | ACD_O bias
27:24 | RW | BIAS_6_IQ_PLL_3 | DLL bias
23:20 | RW | BIAS_5_IQ_PLL_4_RX | VCO bias for Rx mode
19:16 | RW | BIAS_5_IQ_PLL_4_TX | VCO bias for Tx mode
15:12 | RW | BIAS_4_IQ_PLL_2 | Sub-band comparator bias
11:8 | RW | BIAS_4_IQ_PLL_1 | Dynamic divider bias
7:4 | RW | BIAS_3_IQ_RXTX_8 | IFA ctrl_c bias
3:0 | RW | BIAS_3_IQ_RXTX_7 | IFA ctrl_r bias

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:28 | BIAS_6_IQ_BB_0 | BIAS_6_IQ_BB_0_DEFAULT |  | 0x7*
27:24 | BIAS_6_IQ_PLL_3 | BIAS_6_IQ_PLL_3_DEFAULT |  | 0x7*
23:20 | BIAS_5_IQ_PLL_4_RX | BIAS_5_IQ_PLL_4_RX_DEFAULT |  | 0x8*
19:16 | BIAS_5_IQ_PLL_4_TX | BIAS_5_IQ_PLL_4_TX_DEFAULT |  | 0xA*
15:12 | BIAS_4_IQ_PLL_2 | BIAS_4_IQ_PLL_2_DEFAULT |  | 0x7*
11:8 | BIAS_4_IQ_PLL_1 | BIAS_4_IQ_PLL_1_DEFAULT |  | 0x4*
7:4 | BIAS_3_IQ_RXTX_8 | BIAS_3_IQ_RXTX_8_DEFAULT |  | 0x7*
3:0 | BIAS_3_IQ_RXTX_7 | BIAS_3_IQ_RXTX_7_DEFAULT |  | 0x7*