### BB_SPIPTRCNTL3

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
29:16 | RW | CTESAMPPTR | Pointer to the CTE sampling indication sequence address section
13:0 | RW | RXPKTTYPPTR | Pointer to the received packet type indication sequence address section

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
29:16 | CTESAMPPTR | CTESAMPPTR_0 |  | 0x0*
13:0 | RXPKTTYPPTR | RXPKTTYPPTR_0 |  | 0x0*