### RF_REG0C

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:16 | RW | ADDRESS_ADDRESS | Address of the node (banked)
11 | RW | ADDRESS_CONF_ADDRESS_LEN | Address length selection (banked)
10 | RW | ADDRESS_CONF_EN_ADDRESS_RX_BR | Broadcast address detection in Rx mode (banked)
9 | RW | ADDRESS_CONF_EN_ADDRESS_RX | Address detection in Rx mode (banked)
8 | RW | ADDRESS_CONF_EN_ADDRESS_TX | Address insertion in Tx mode (banked)
7:0 | RW | PREAMBLE_LENGTH_PREAMBLE_LEN | Length of the preamble -1 (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:16 | ADDRESS_ADDRESS | ADDRESS_ADDRESS_DEFAULT |  | 0x0*
11 | ADDRESS_CONF_ADDRESS_LEN | ADDRESS_CONF_ADDRESS_LEN_8 | Address length is 8 bits | 0x0*
|  | ADDRESS_CONF_ADDRESS_LEN_16 | Address length is 16 bits | 0x1
10 | ADDRESS_CONF_EN_ADDRESS_RX_BR | ADDRESS_CONF_EN_ADDRESS_RX_BR_DISABLE | Disable the broadcast address detection on Rx | 0x0*
|  | ADDRESS_CONF_EN_ADDRESS_RX_BR_ENABLE | Enable the broadcast address detection on Rx | 0x1
9 | ADDRESS_CONF_EN_ADDRESS_RX | ADDRESS_CONF_EN_ADDRESS_RX_DISABLE | Disable the address detection on Rx | 0x0*
|  | ADDRESS_CONF_EN_ADDRESS_RX_ENABLE | Enable the address detection on Rx | 0x1
8 | ADDRESS_CONF_EN_ADDRESS_TX | ADDRESS_CONF_EN_ADDRESS_TX_DISABLE | Disable the address insertion on Tx | 0x0*
|  | ADDRESS_CONF_EN_ADDRESS_TX_ENABLE | Enable the address insertion on Tx | 0x1
7:0 | PREAMBLE_LENGTH_PREAMBLE_LEN | PREAMBLE_LENGTH_PREAMBLE_LEN_DEFAULT |  | 0x0*