### NVIC_ICER1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
24 | RW | DMA3 | DMA3 interrupt clear enable
23 | RW | DMA2 | DMA2 interrupt clear enable
22 | RW | DMA1 | DMA1 interrupt clear enable
21 | RW | DMA0 | DMA0 interrupt clear enable
20 | RW | ACCESS_ERROR | ACCESS_ERROR interrupt clear enable
19 | RW | FLASH0_ECC | FLASH0_ECC interrupt clear enable
18 | RW | FLASH0_COPY | FLASH0_COPY interrupt clear enable
17 | RW | RF_RXFIFO | RF_RXFIFO interrupt clear enable
16 | RW | RF_TXFIFO | RF_TXFIFO interrupt clear enable
15 | RW | RF_SYNC | RF_SYNC interrupt clear enable
14 | RW | RF_IRQ_RECEIVED | RF_IRQ_RECEIVED interrupt clear enable
13 | RW | RF_RXSTOP | RF_RXSTOP interrupt clear enable
12 | RW | RF_TX | RF_TX interrupt clear enable
11 | RW | TOF | TOF interrupt clear enable
10 | RW | BLE_COEX_RX_TX | BLE_COEX_RX_TX interrupt clear enable
9 | RW | BLE_COEX_IN_PROCESS | BLE_COEX_IN_PROCESS interrupt clear enable
8 | RW | BLE_ERROR | BLE_ERROR interrupt clear enable
7 | RW | BLE_FIFO | BLE_FIFO interrupt clear enable
6 | RW | BLE_HSLOT | BLE_HSLOT interrupt clear enable
5 | RW | BLE_SLP | BLE_SLP interrupt clear enable
4 | RW | BLE_CRYPT | BLE_CRYPT interrupt clear enable
3 | RW | BLE_TIMESTAMP_TGT2 | BLE_TIMESTAMP_TGT2 interrupt clear enable
2 | RW | BLE_TIMESTAMP_TGT1 | BLE_TIMESTAMP_TGT1 interrupt clear enable
1 | RW | BLE_FINETGT | BLE_FINETGT interrupt clear enable
0 | RW | BLE_SW | BLE_SW interrupt clear enable

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
24 | DMA3 | NVIC_DMA3_INT_DISABLE | Disable the DMA3 interrupt | 0x0
23 | DMA2 | NVIC_DMA2_INT_DISABLE | Disable the DMA2 interrupt | 0x1
22 | DMA1 | NVIC_DMA1_INT_DISABLE | Disable the DMA1 interrupt | 0x1
21 | DMA0 | NVIC_DMA0_INT_DISABLE | Disable the DMA0 interrupt | 0x1
20 | ACCESS_ERROR | NVIC_ACCESS_ERROR_INT_DISABLE | Disable the ACCESS_ERROR interrupt | 0x1
19 | FLASH0_ECC | NVIC_FLASH0_ECC_INT_DISABLE | Disable the FLASH0_ECC interrupt | 0x1
18 | FLASH0_COPY | NVIC_FLASH0_COPY_INT_DISABLE | Disable the FLASH0_COPY interrupt | 0x1
17 | RF_RXFIFO | NVIC_RF_RXFIFO_INT_DISABLE | Disable the RF_RXFIFO interrupt | 0x1
16 | RF_TXFIFO | NVIC_RF_TXFIFO_INT_DISABLE | Disable the RF_TXFIFO interrupt | 0x1
15 | RF_SYNC | NVIC_RF_SYNC_INT_DISABLE | Disable the RF_SYNC interrupt | 0x1
14 | RF_IRQ_RECEIVED | NVIC_RF_IRQ_RECEIVED_INT_DISABLE | Disable the RF_IRQ_RECEIVED interrupt | 0x1
13 | RF_RXSTOP | NVIC_RF_RXSTOP_INT_DISABLE | Disable the RF_RXSTOP interrupt | 0x1
12 | RF_TX | NVIC_RF_TX_INT_DISABLE | Disable the RF_TX interrupt | 0x1
11 | TOF | NVIC_TOF_INT_DISABLE | Disable the TOF interrupt | 0x1
10 | BLE_COEX_RX_TX | NVIC_BLE_COEX_RX_TX_INT_DISABLE | Disable the BLE_COEX_RX_TX interrupt | 0x1
9 | BLE_COEX_IN_PROCESS | NVIC_BLE_COEX_IN_PROCESS_INT_DISABLE | Disable the BLE_COEX_IN_PROCESS interrupt | 0x1
8 | BLE_ERROR | NVIC_BLE_ERROR_INT_DISABLE | Disable the BLE_ERROR interrupt | 0x1
7 | BLE_FIFO | NVIC_BLE_FIFO_INT_DISABLE | Disable the BLE_FIFO interrupt | 0x1
6 | BLE_HSLOT | NVIC_BLE_HSLOT_INT_DISABLE | Disable the BLE_HSLOT interrupt | 0x1
5 | BLE_SLP | NVIC_BLE_SLP_INT_DISABLE | Disable the BLE_SLP interrupt | 0x1
4 | BLE_CRYPT | NVIC_BLE_CRYPT_INT_DISABLE | Disable the BLE_CRYPT interrupt | 0x1
3 | BLE_TIMESTAMP_TGT2 | NVIC_BLE_TIMESTAMP_TGT2_INT_DISABLE | Disable the BLE_TIMESTAMP_TGT2 interrupt | 0x1
2 | BLE_TIMESTAMP_TGT1 | NVIC_BLE_TIMESTAMP_TGT1_INT_DISABLE | Disable the BLE_TIMESTAMP_TGT1 interrupt | 0x1
1 | BLE_FINETGT | NVIC_BLE_FINETGT_INT_DISABLE | Disable the BLE_FINETGT interrupt | 0x1
0 | BLE_SW | NVIC_BLE_SW_INT_DISABLE | Disable the BLE_SW interrupt | 0x1