### RF_REG34

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
29:24 | RW | CLK_RECOVERY_CLK_RECOV_CORR | Number of samples that covers the clock recovery correlator
23:16 | RW | CLK_RECOVERY_CLK_AB_LIMIT | Time constant for switch the clock phase if chosen wrong in clk recovery algorithm
15 | RW | TX_PRE_DIST_EN_PRE_DIST | Tx pre-distortion filter (banked)
13:8 | RW | TX_PRE_DIST_PRE_DIST_B0 | Coefficient b0 of the Tx pre-distortion filter (banked)
5:0 | RW | TX_PRE_DIST_PRE_DIST_A0 | Coefficient a0 of the Tx pre-distortion filter (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
29:24 | CLK_RECOVERY_CLK_RECOV_CORR | CLK_RECOVERY_CLK_RECOV_CORR_DEFAULT |  | 0x4*
23:16 | CLK_RECOVERY_CLK_AB_LIMIT | CLK_RECOVERY_CLK_AB_LIMIT_DEFAULT |  | 0x80*
15 | TX_PRE_DIST_EN_PRE_DIST | TX_PRE_DIST_EN_PRE_DIST_DISABLE | Disable the Tx pre-distortion filter | 0x0
|  | TX_PRE_DIST_EN_PRE_DIST_ENABLE | Enable the Tx pre-distortion filter | 0x1*
13:8 | TX_PRE_DIST_PRE_DIST_B0 | TX_PRE_DIST_PRE_DIST_B0_DEFAULT | The coefficient value is the (pre_dist_b0+64)/128 | 0x2E*
5:0 | TX_PRE_DIST_PRE_DIST_A0 | TX_PRE_DIST_PRE_DIST_A0_DEFAULT | The coefficient value is the (pre_dist_a0+64)/128 | 0x2F*