### FLASH_IF_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | R | TRIMMED_STATUS | Flash trimming status
30 | R | ISOLATE_STATUS | Flash isolate status
29 | R | PROG_SEQ_DATA_REQ | Request new data while in sequential program mode
28 | R | BUSY | Flash interface busy status bit
27 | R | DATA_RED2_W_UNLOCK | Flash Data array RED2 write unlock status bit
26 | R | DATA_RED1_W_UNLOCK | Flash Data array RED1 write unlock status bit
25 | R | CODE_RED2_W_UNLOCK | Flash Code array RED2 write unlock status bit
24 | R | CODE_RED1_W_UNLOCK | Flash Code array RED1 write unlock status bit
22 | R | NVR7_W_UNLOCK | Flash NVR7 write unlock status bit
21 | R | NVR6_W_UNLOCK | Flash NVR6 write unlock status bit
20 | R | NVR5_W_UNLOCK | Flash NVR5 write unlock status bit
19 | R | NVR4_W_UNLOCK | Flash NVR4 write unlock status bit
18 | R | NVR3_W_UNLOCK | Flash NVR3 write unlock status bit
17 | R | NVR2_W_UNLOCK | Flash NVR2 write unlock status bit
16 | R | NVR1_W_UNLOCK | Flash NVR1 write unlock status bit
15 | R | NVR0_W_UNLOCK | Flash NVR0 write unlock status bit
11 | R | DATA_A_35K_TO_40K_W_UNLOCK | Write unlock status bit of the part 35K to 40K of the Flash MAIN Data array
10 | R | DATA_A_30K_TO_35K_W_UNLOCK | Write unlock status bit of the part 30K to 35K of the Flash MAIN Data array
9 | R | DATA_A_25K_TO_30K_W_UNLOCK | Write unlock status bit of the part 25K to 30K of the Flash MAIN Data array
8 | R | DATA_A_20K_TO_25K_W_UNLOCK | Write unlock status bit of the part 20K to 25K of the Flash MAIN Data array
7 | R | DATA_A_15K_TO_20K_W_UNLOCK | Write unlock status bit of the part 15K to 20K of the Flash MAIN Data array
6 | R | DATA_A_10K_TO_15K_W_UNLOCK | Write unlock status bit of the part 10K to 15K of the Flash MAIN Data array
5 | R | DATA_A_5K_TO_10K_W_UNLOCK | Write unlock status bit of the part 5K to 10K of the Flash MAIN Data array
4 | R | DATA_A_0K_TO_5K_W_UNLOCK | Write unlock status bit of the part 0K to 5K of the Flash MAIN Data array
3 | R | CODE_A_66K_TO_88K_W_UNLOCK | Write unlock status bit of the part 66K to 88K of the Flash MAIN Code array
2 | R | CODE_A_44K_TO_66K_W_UNLOCK | Write unlock status bit of the part 44K to 66K of the Flash MAIN Code array
1 | R | CODE_A_22K_TO_44K_W_UNLOCK | Write unlock status bit of the part 22K to 44K of the Flash MAIN Code array
0 | R | CODE_A_0K_TO_22K_W_UNLOCK | Write unlock status bit of the part 0K to 22K of the Flash MAIN Code array

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | TRIMMED_STATUS | FLASH_UNTRIMMED | All MNVR CBD0-CDB7 contents are equal to 0xFFFF. Flash untrimmed. | 0x0*
|  | FLASH_TRIMMED | Some registers CBD0-CBD7 contents are not equal to 0xFFFF. Flash trimmed. | 0x1
30 | ISOLATE_STATUS | FLASH_ACCESSIBLE | Flash can be accessed (isolation inactive) | 0x0
|  | FLASH_ISOLATE | Flash cannot be accessed (isolation active) | 0x1*
29 | PROG_SEQ_DATA_REQ | FLASH_PROG_SEQ_IDLE | No new data is requested by a Sequential Program sequence. | 0x0*
|  | FLASH_PROG_SEQ_REQ_NEW_DATA | New data is requested by a Sequential Program sequence. | 0x1
28 | BUSY | FLASH_IF_IDLE | Indicates that the Flash interface is ready. | 0x0*
|  | FLASH_IF_BUSY | Indicates that the Flash interface is busy. | 0x1
27 | DATA_RED2_W_UNLOCK | FLASH_DATA_RED2_W_LOCKED | Indicates that the Flash Data array RED2 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_DATA_RED2_W_UNLOCKED | Indicates that the Flash Data array RED2 sector can be write accessed by the Flash interface | 0x1
26 | DATA_RED1_W_UNLOCK | FLASH_DATA_RED1_W_LOCKED | Indicates that the Flash Data array RED1 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_DATA_RED1_W_UNLOCKED | Indicates that the Flash Data array RED1 sector can be write accessed by the Flash interface | 0x1
25 | CODE_RED2_W_UNLOCK | FLASH_CODE_RED2_W_LOCKED | Indicates that the Flash Code array RED2 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_CODE_RED2_W_UNLOCKED | Indicates that the Flash Code array RED2 sector can be write accessed by the Flash interface | 0x1
24 | CODE_RED1_W_UNLOCK | FLASH_CODE_RED1_W_LOCKED | Indicates that the Flash Code array RED1 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_CODE_RED1_W_UNLOCKED | Indicates that the Flash Code array RED1 sector can be write accessed by the Flash interface | 0x1
22 | NVR7_W_UNLOCK | FLASH_NVR7_W_LOCKED | Indicates that the Flash NVR7 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_NVR7_W_UNLOCKED | Indicates that the Flash NVR7 sector can be write accessed by the Flash interface | 0x1
21 | NVR6_W_UNLOCK | FLASH_NVR6_W_LOCKED | Indicates that the Flash NVR6 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_NVR6_W_UNLOCKED | Indicates that the Flash NVR6 sector can be write accessed by the Flash interface | 0x1
20 | NVR5_W_UNLOCK | FLASH_NVR5_W_LOCKED | Indicates that the Flash NVR5 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_NVR5_W_UNLOCKED | Indicates that the Flash NVR5 sector can be write accessed by the Flash interface | 0x1
19 | NVR4_W_UNLOCK | FLASH_NVR4_W_LOCKED | Indicates that the Flash NVR4 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_NVR4_W_UNLOCKED | Indicates that the Flash NVR4 sector can be write accessed by the Flash interface | 0x1
18 | NVR3_W_UNLOCK | FLASH_NVR3_W_LOCKED | Indicates that the Flash NVR3 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_NVR3_W_UNLOCKED | Indicates that the Flash NVR3 sector can be write accessed by the Flash interface | 0x1
17 | NVR2_W_UNLOCK | FLASH_NVR2_W_LOCKED | Indicates that the Flash NVR2 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_NVR2_W_UNLOCKED | Indicates that the Flash NVR2 sector can be write accessed by the Flash interface | 0x1
16 | NVR1_W_UNLOCK | FLASH_NVR1_W_LOCKED | Indicates that the Flash NVR1 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_NVR1_W_UNLOCKED | Indicates that the Flash NVR1 sector can be write accessed by the Flash interface | 0x1
15 | NVR0_W_UNLOCK | FLASH_NVR0_W_LOCKED | Indicates that the Flash NVR0 sector is protected against write accesses by the Flash interface | 0x0*
|  | FLASH_NVR0_W_UNLOCKED | Indicates that the Flash NVR0 sector can be write accessed by the Flash interface | 0x1
11 | DATA_A_35K_TO_40K_W_UNLOCK | DATA_A_35K_TO_40K_W_LOCKED | Indicates that the part 35K to 40K of the Flash MAIN Data array is protected against write accesses by the Flash interface | 0x0*
|  | DATA_A_35K_TO_40K_W_UNLOCKED | Indicates that the part 35K to 40K of the Flash MAIN Data array can be write accessed by the Flash interface | 0x1
10 | DATA_A_30K_TO_35K_W_UNLOCK | DATA_A_30K_TO_35K_W_LOCKED | Indicates that the part 30K to 35K of the Flash MAIN Data array is protected against write accesses by the Flash interface | 0x0*
|  | DATA_A_30K_TO_35K_W_UNLOCKED | Indicates that the part 30K to 35K of the Flash MAIN Data array can be write accessed by the Flash interface | 0x1
9 | DATA_A_25K_TO_30K_W_UNLOCK | DATA_A_25K_TO_30K_W_LOCKED | Indicates that the part 25K to 30K of the Flash MAIN Data array is protected against write accesses by the Flash interface | 0x0*
|  | DATA_A_25K_TO_30K_W_UNLOCKED | Indicates that the part 25K to 30K of the Flash MAIN Data array can be write accessed by the Flash interface | 0x1
8 | DATA_A_20K_TO_25K_W_UNLOCK | DATA_A_20K_TO_25K_W_LOCKED | Indicates that the part 20K to 25K of the Flash MAIN Data array is protected against write accesses by the Flash interface | 0x0*
|  | DATA_A_20K_TO_25K_W_UNLOCKED | Indicates that the part 20K to 25K of the Flash MAIN Data array can be write accessed by the Flash interface | 0x1
7 | DATA_A_15K_TO_20K_W_UNLOCK | DATA_A_15K_TO_20K_W_LOCKED | Indicates that the part 15K to 20K of the Flash MAIN Data array is protected against write accesses by the Flash interface | 0x0*
|  | DATA_A_15K_TO_20K_W_UNLOCKED | Indicates that the part 15K to 20K of the Flash MAIN Data array can be write accessed by the Flash interface | 0x1
6 | DATA_A_10K_TO_15K_W_UNLOCK | DATA_A_10K_TO_15K_W_LOCKED | Indicates that the part 10K to 15K of the Flash MAIN Data array is protected against write accesses by the Flash interface | 0x0*
|  | DATA_A_10K_TO_15K_W_UNLOCKED | Indicates that the part 10K to 15K of the Flash MAIN Data array can be write accessed by the Flash interface | 0x1
5 | DATA_A_5K_TO_10K_W_UNLOCK | DATA_A_5K_TO_10K_W_LOCKED | Indicates that the part 5K to 10K of the Flash MAIN Data array is protected against write accesses by the Flash interface | 0x0*
|  | DATA_A_5K_TO_10K_W_UNLOCKED | Indicates that the part 5K to 10K of the Flash MAIN Data array can be write accessed by the Flash interface | 0x1
4 | DATA_A_0K_TO_5K_W_UNLOCK | DATA_A_0K_TO_5K_W_LOCKED | Indicates that the part 0K to 5K of the Flash MAIN Data array is protected against write accesses by the Flash interface | 0x0*
|  | DATA_A_0K_TO_5K_W_UNLOCKED | Indicates that the part 0K to 5K of the Flash MAIN Data array can be write accessed by the Flash interface | 0x1
3 | CODE_A_66K_TO_88K_W_UNLOCK | CODE_A_66K_TO_88K_W_LOCKED | Indicates that the part 66K to 88K of the Flash MAIN Code array is protected against write accesses by the Flash interface | 0x0*
|  | CODE_A_66K_TO_88K_W_UNLOCKED | Indicates that the part 66K to 88K of the Flash MAIN Code array can be write accessed by the Flash interface | 0x1
2 | CODE_A_44K_TO_66K_W_UNLOCK | CODE_A_44K_TO_66K_W_LOCKED | Indicates that the part 44K to 66K of the Flash MAIN Code array is protected against write accesses by the Flash interface | 0x0*
|  | CODE_A_44K_TO_66K_W_UNLOCKED | Indicates that the part 44K to 66K of the Flash MAIN Code array can be write accessed by the Flash interface | 0x1
1 | CODE_A_22K_TO_44K_W_UNLOCK | CODE_A_22K_TO_44K_W_LOCKED | Indicates that the part 22K to 44K of the Flash MAIN Code array is protected against write accesses by the Flash interface | 0x0*
|  | CODE_A_22K_TO_44K_W_UNLOCKED | Indicates that the part 22K to 44K of the Flash MAIN Code array can be write accessed by the Flash interface | 0x1
0 | CODE_A_0K_TO_22K_W_UNLOCK | CODE_A_0K_TO_22K_W_LOCKED | Indicates that the part 0K to 22K of the Flash MAIN Code array is protected against write accesses by the Flash interface | 0x0*
|  | CODE_A_0K_TO_22K_W_UNLOCKED | Indicates that the part 0K to 22K of the Flash MAIN Code array can be write accessed by the Flash interface | 0x1