### GPIO_INPUT_DATA

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
15:0 | R | DATA | GPIO[15:0] read data

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
15:0 | DATA | GPIO0_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO1_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO2_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO3_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO4_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO5_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO6_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO7_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO8_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO9_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO10_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO11_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO12_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO13_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO14_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO15_IN_LOW | GPIO pad is low | 0x0*
|  | GPIO0_IN_HIGH | GPIO pad is high | 0x1
|  | GPIO1_IN_HIGH | GPIO pad is high | 0x2
|  | GPIO2_IN_HIGH | GPIO pad is high | 0x4
|  | GPIO3_IN_HIGH | GPIO pad is high | 0x8
|  | GPIO4_IN_HIGH | GPIO pad is high | 0x10
|  | GPIO5_IN_HIGH | GPIO pad is high | 0x20
|  | GPIO6_IN_HIGH | GPIO pad is high | 0x40
|  | GPIO7_IN_HIGH | GPIO pad is high | 0x80
|  | GPIO8_IN_HIGH | GPIO pad is high | 0x100
|  | GPIO9_IN_HIGH | GPIO pad is high | 0x200
|  | GPIO10_IN_HIGH | GPIO pad is high | 0x400
|  | GPIO11_IN_HIGH | GPIO pad is high | 0x800
|  | GPIO12_IN_HIGH | GPIO pad is high | 0x1000
|  | GPIO13_IN_HIGH | GPIO pad is high | 0x2000
|  | GPIO14_IN_HIGH | GPIO pad is high | 0x4000
|  | GPIO15_IN_HIGH | GPIO pad is high | 0x8000