### RF_REG52

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | ACCESS_ADDRESS | Remapped register of PATTERN
23:16 | RW | FSM_MODE_RM_RX | Remapped register of FSM_MODE
15:8 | RW | CHANNEL_RM_RX | Remapped register of CHANNEL
7:0 | RW | RATE_RX | Remapped register of BANK

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | ACCESS_ADDRESS | ACCESS_ADDRESS_DEFAULT | The remapped registers are accessible over SPI only | 0x0*
23:16 | FSM_MODE_RM_RX | FSM_MODE_RM_RX_DEFAULT | The remapped registers are accessible over SPI only | 0x0*
15:8 | CHANNEL_RM_RX | CHANNEL_RM_RX_DEFAULT | The remapped registers are accessible over SPI only | 0x0*
7:0 | RATE_RX | RATE_RX_DEFAULT | The remapped registers are accessible over SPI only | 0x0*