### SYSCTRL_MEM_ACCESS_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
29:24 | RW | WAKEUP_ADDR_PACKED | Wakeup restore address in packed 6-bit format. When written, SYSCTRL_WAKEUP_ADDR is updated. This field reads back as zero when SYSCTRL_WAKEUP_ADDR does not point to an enabled RAM instance.
17:16 | RW | BB_DRAM_ACCESS | Baseband DRAM[1:0] access configuration
15:8 | RW | DRAM_ACCESS | DRAM[7:0] access configuration
1 | RW | FLASH_ACCESS | FLASH[0:0] access configuration
0 | RW | PROM_ACCESS | PROM access configuration

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
17:16 | BB_DRAM_ACCESS | BB_DRAM0_ACCESS_DISABLE | Baseband DRAM0 access disabled | 0x0*
|  | BB_DRAM1_ACCESS_DISABLE | Baseband DRAM1 access disabled | 0x0*
|  | BB_DRAM0_ACCESS_ENABLE | Baseband DRAM0 access enabled | 0x1
|  | BB_DRAM1_ACCESS_ENABLE | Baseband DRAM1 access enabled | 0x2
15:8 | DRAM_ACCESS | DRAM0_ACCESS_DISABLE | DRAM0 access disabled | 0x0
|  | DRAM1_ACCESS_DISABLE | DRAM1 access disabled | 0x0
|  | DRAM2_ACCESS_DISABLE | DRAM2 access disabled | 0x0
|  | DRAM3_ACCESS_DISABLE | DRAM3 access disabled | 0x0
|  | DRAM4_ACCESS_DISABLE | DRAM4 access disabled | 0x0
|  | DRAM5_ACCESS_DISABLE | DRAM5 access disabled | 0x0
|  | DRAM6_ACCESS_DISABLE | DRAM6 access disabled | 0x0
|  | DRAM7_ACCESS_DISABLE | DRAM7 access disabled | 0x0
|  | DRAM0_ACCESS_ENABLE | DRAM0 access enabled | 0x1*
|  | DRAM1_ACCESS_ENABLE | DRAM1 access enabled | 0x2
|  | DRAM2_ACCESS_ENABLE | DRAM2 access enabled | 0x4
|  | DRAM3_ACCESS_ENABLE | DRAM3 access enabled | 0x8
|  | DRAM4_ACCESS_ENABLE | DRAM4 access enabled | 0x10
|  | DRAM5_ACCESS_ENABLE | DRAM5 access enabled | 0x20
|  | DRAM6_ACCESS_ENABLE | DRAM6 access enabled | 0x40
|  | DRAM7_ACCESS_ENABLE | DRAM7 access enabled | 0x80
1 | FLASH_ACCESS | FLASH0_ACCESS_DISABLE | FLASH0 access disabled | 0x0*
|  | FLASH0_ACCESS_ENABLE | FLASH0 access enabled | 0x1
0 | PROM_ACCESS | PROM_ACCESS_DISABLE | PROM access disabled | 0x0
|  | PROM_ACCESS_ENABLE | PROM access enabled | 0x1*