## CMSIS GPIO Driver Macro Definition Documentation

### ARM_GPIO_API_VERSION

#define ARM_GPIO_API_VERSION ARM_DRIVER_VERSION_MAJOR_MINOR(1,0)

GPIO API version.

Location: Driver_GPIO.h:71

### GPIO_EVENT_0_IRQ

#define GPIO_EVENT_0_IRQ (1UL << 0)

GPIO Event.

GPIO0 interrupt event value

Location: Driver_GPIO.h:344

### GPIO_EVENT_1_IRQ

#define GPIO_EVENT_1_IRQ (1UL << 1)

GPIO1 interrupt event value.

Location: Driver_GPIO.h:345

### GPIO_EVENT_2_IRQ

#define GPIO_EVENT_2_IRQ (1UL << 2)

GPIO2 interrupt event value.

Location: Driver_GPIO.h:346

### GPIO_EVENT_3_IRQ

#define GPIO_EVENT_3_IRQ (1UL << 3)

GPIO3 interrupt event value.

Location: Driver_GPIO.h:347