### LSAD_DUTY

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
15:14 | RW | CH7_DUTY_CFG | Input to channel 7 duty config
13:12 | RW | CH6_DUTY_CFG | Input to channel 6 duty config
11:10 | RW | CH5_DUTY_CFG | Input to channel 5 duty config
9:8 | RW | CH4_DUTY_CFG | Input to channel 4 duty config
7:6 | RW | CH3_DUTY_CFG | Input to channel 3 duty config
5:4 | RW | CH2_DUTY_CFG | Input to channel 2 duty config
3:2 | RW | CH1_DUTY_CFG | Input to channel 1 duty config
1:0 | RW | CH0_DUTY_CFG | Input to channel 0 duty config

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
15:14 | CH7_DUTY_CFG | INPUT_TO_CH7_PERMANENT | Input always connected to channel | 0x0*
|  | INPUT_TO_CH7_DUTY | Input only connected to the channel during this conversion | 0x1
|  | INPUT_TO_CH7_RESERVED | reserved - same as 0x0 | 0x2
|  | INPUT_TO_CH7_PRE_CONV | Input connected to the channel during this conversion and the previous conversion | 0x3
13:12 | CH6_DUTY_CFG | INPUT_TO_CH6_PERMANENT | Input always connected to channel | 0x0*
|  | INPUT_TO_CH6_DUTY | Input only connected to the channel during this conversion | 0x1
|  | INPUT_TO_CH6_RESERVED | reserved - same as 0x0 | 0x2
|  | INPUT_TO_CH6_PRE_CONV | Input connected to the channel during this conversion and the previous conversion | 0x3
11:10 | CH5_DUTY_CFG | INPUT_TO_CH5_PERMANENT | Input always connected to channel | 0x0*
|  | INPUT_TO_CH5_DUTY | Input only connected to the channel during this conversion | 0x1
|  | INPUT_TO_CH5_RESERVED | reserved - same as 0x0 | 0x2
|  | INPUT_TO_CH5_PRE_CONV | Input connected to the channel during this conversion and the previous conversion | 0x3
9:8 | CH4_DUTY_CFG | INPUT_TO_CH4_PERMANENT | Input always connected to channel | 0x0*
|  | INPUT_TO_CH4_DUTY | Input only connected to the channel during this conversion | 0x1
|  | INPUT_TO_CH4_RESEREVED | reserved - same as 0x0 | 0x2
|  | INPUT_TO_CH4_PRE_CONV | Input connected to the channel during this conversion and the previous conversion | 0x3
7:6 | CH3_DUTY_CFG | INPUT_TO_CH3_PERMANENT | Input always connected to channel | 0x0*
|  | INPUT_TO_CH3_DUTY | Input only connected to the channel during this conversion | 0x1
|  | INPUT_TO_CH3_RESERVED | reserved - same as 0x0 | 0x2
|  | INPUT_TO_CH3_PRE_CONV | Input connected to the channel during this conversion and the previous conversion | 0x3
5:4 | CH2_DUTY_CFG | INPUT_TO_CH2_PERMANENT | Input always connected to channel | 0x0*
|  | INPUT_TO_CH2_DUTY | Input only connected to the channel during this conversion | 0x1
|  | INPUT_TO_CH2_RESERVED | reserved - same as 0x0 | 0x2
|  | INPUT_TO_CH2_PRE_CONV | Input connected to the channel during this conversion and the previous conversion | 0x3
3:2 | CH1_DUTY_CFG | INPUT_TO_CH1_PERMANENT | Input always connected to channel | 0x0*
|  | INPUT_TO_CH1_DUTY | Input only connected to the channel during this conversion | 0x1
|  | INPUT_TO_CH1_RESERVED | reserved - same as 0x0 | 0x2
|  | INPUT_TO_CH1_PRE_CONV | Input connected to the channel during this conversion and the previous conversion | 0x3
1:0 | CH0_DUTY_CFG | INPUT_TO_CH0_PERMANENT | Input always connected to channel | 0x0*
|  | INPUT_TO_CH0_DUTY | Input only connected to the channel during this conversion | 0x1
|  | INPUT_TO_CH0_RESERVED | reserved - same as 0x0 | 0x2
|  | INPUT_TO_CH0_PRE_CONV | Input connected to the channel during this conversion and the previous conversion | 0x3