### ACS_VDDFLASH_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
24 | R | READY | Supply ready
11 | RW | MASK_READY | Apply a mask to reset logic to ignore VDDFLASH ready signal
10 | RW | SOFT_START | Current limiter threshold setting
9 | RW | ENABLE_LIMITER | Enable current limiter circuit
8 | RW | ENABLE | Enable control
5:0 | RW | VTRIM | Output voltage trimming configuration in 25 mV steps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
24 | READY | VDDFLASH_NOT_READY | Supply voltage not ready | 0x0*
|  | VDDFLASH_READY | Supply voltage ready | 0x1
11 | MASK_READY | VDDFLASH_USE_READY | Reset logic use VDDFLASH ready | 0x0*
|  | VDDFLASH_MASK_READY | Reset ignore VDDFLASH ready | 0x1
10 | SOFT_START | VDDFLASH_LIMITER_70MA | Limiter current threshold at 70mA | 0x0
|  | VDDFLASH_LIMITER_4MA | Limiter current threshold at 4mA | 0x1*
9 | ENABLE_LIMITER | VDDFLASH_LIMITER_DISABLE | Disable the VDDFLASH regulator current limiter circuit | 0x0
|  | VDDFLASH_LIMITER_ENABLE | Enable the VDDFLASH regulator current limiter circuit | 0x1*
8 | ENABLE | VDDFLASH_DISABLE | Disable the VDDFLASH regulator | 0x0
|  | VDDFLASH_ENABLE | Enable the VDDFLASH regulator | 0x1*
5:0 | VTRIM | VDDFLASH_TRIM_0P750V | 0.750V | 0x0
|  | VDDFLASH_TRIM_0P775V | 0.775V | 0x1
|  | VDDFLASH_TRIM_1P725V | 1.725V | 0x27
|  | VDDFLASH_TRIM_1P750V | 1.750V | 0x28*
|  | VDDFLASH_TRIM_1P775V | 1.775V | 0x29
|  | VDDFLASH_TRIM_2P300V | 2.300V | 0x3E
|  | VDDFLASH_TRIM_2P325V | 2.325V | 0x3F