### RF_BIAS_7_9

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:28 | RW | BIAS_9_IQ_BB_6 | Peak detector threshold bias 0
27:24 | RW | BIAS_9_IQ_BB_5 | Peak detector bias
23:20 | RW | SWCAP_FSM_SB_CAP_RX | VCO subband selection (FSM in Rx mode)
19:16 | RW | SWCAP_FSM_SB_CAP_TX | VCO subband selection (FSM in Tx mode)
15:12 | RW | BIAS_8_IQ_BB_4 | RSSI_D bias
11:8 | RW | BIAS_8_IQ_BB_3 | RSSI_G bias
7:4 | RW | BIAS_7_IQ_BB_2 | ACD_L bias
3:0 | RW | BIAS_7_IQ_BB_1 | ACD_C bias

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:28 | BIAS_9_IQ_BB_6 | BIAS_9_IQ_BB_6_DEFAULT |  | 0x9*
27:24 | BIAS_9_IQ_BB_5 | BIAS_9_IQ_BB_5_DEFAULT |  | 0x5*
23:20 | SWCAP_FSM_SB_CAP_RX | SWCAP_FSM_SB_CAP_RX_DEFAULT |  | 0x0*
19:16 | SWCAP_FSM_SB_CAP_TX | SWCAP_FSM_SB_CAP_TX_DEFAULT |  | 0x0*
15:12 | BIAS_8_IQ_BB_4 | BIAS_8_IQ_BB_4_DEFAULT |  | 0x9*
11:8 | BIAS_8_IQ_BB_3 | BIAS_8_IQ_BB_3_DEFAULT |  | 0xF*
7:4 | BIAS_7_IQ_BB_2 | BIAS_7_IQ_BB_2_DEFAULT |  | 0x6*
3:0 | BIAS_7_IQ_BB_1 | BIAS_7_IQ_BB_1_DEFAULT |  | 0x6*