### ACS_RTC_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
18 | R | ENABLE_CLOCK_EVENT_STATUS | Status of the RTC clock event enable
17 | R | ENABLE_ALARM_EVENT_STATUS | Status of the RTC alarm event enable
16 | R | ENABLE_STATUS | Status of the RTC enable
7 | W | FORCE_CLOCK | Force a clock on RTC timer (Test Purpose)
6 | W | DISABLE_CLOCK_EVENT | Disable clock event and its interrupt
5 | W | ENABLE_CLOCK_EVENT | Enable clock event and its interrupt
4 | W | DISABLE_ALARM_EVENT | Disable alarm event and its interrupt
3 | W | ENABLE_ALARM_EVENT | Enable alarm event and its interrupt
2 | W | RESET | Reset the RTC timer
1 | W | DISABLE | Disable counter and RTC interrupt every 1s
0 | W | ENABLE | Enable counter and RTC interrupt every 1s

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
18 | ENABLE_CLOCK_EVENT_STATUS | RTC_CLOCK_EVENT_IS_DISABLED | The RTC clock event is disabled | 0x0*
|  | RTC_CLOCK_EVENT_IS_ENABLED | The RTC clock event is enabled | 0x1
17 | ENABLE_ALARM_EVENT_STATUS | RTC_ALARM_EVENT_IS_DISABLED | The RTC alarm event is disabled | 0x0*
|  | RTC_ALARM_EVENT_IS_ENABLED | The RTC alarm event is enabled | 0x1
16 | ENABLE_STATUS | RTC_IS_DISABLED | The RTC is disabled | 0x0*
|  | RTC_IS_ENABLED | The RTC is enabled | 0x1
7 | FORCE_CLOCK | RTC_FORCE_CLOCK | Clock the RTC timer (has an effect only if the source clock is low) | 0x1
6 | DISABLE_CLOCK_EVENT | RTC_DISABLE_CLOCK_EVENT | Disable RTC clock event | 0x1
5 | ENABLE_CLOCK_EVENT | RTC_ENABLE_CLOCK_EVENT | Enable RTC clock event | 0x1
4 | DISABLE_ALARM_EVENT | RTC_DISABLE_ALARM_EVENT | Disable RTC alarm event | 0x1
3 | ENABLE_ALARM_EVENT | RTC_ENABLE_ALARM_EVENT | Enable RTC alarm event | 0x1
2 | RESET | RTC_RESET | The RTC counters are reset (prescale and counter) | 0x1
1 | DISABLE | RTC_DISABLE | Disable RTC | 0x1
0 | ENABLE | RTC_ENABLE | Enable RTC | 0x1