### RF_REG4C

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | R | LINK_QUAL_PKT_LINK_QUALITY_PKT | Link quality indicator sampled during the packet reception
23:16 | R | LINK_QUAL_LINK_QUALITY | Instantaneous link quality indicator
15:0 | R | FEI_AFC_FEI_AFC | Frequency error indicator sampled during the AFC

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | LINK_QUAL_PKT_LINK_QUALITY_PKT | LINK_QUAL_PKT_LINK_QUALITY_PKT_DEFAULT |  | 0x0*
23:16 | LINK_QUAL_LINK_QUALITY | LINK_QUAL_LINK_QUALITY_DEFAULT |  | 0x0*
15:0 | FEI_AFC_FEI_AFC | FEI_AFC_FEI_AFC_DEFAULT |  | 0x0*