### BB_BLEMPRIO2

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:28 | RW | BLEMDEFAULT | Set priority value for extended initiating on secondary advertising channels
11:8 | RW | BLEM18 | Set priority value for connection establishment BLE message on secondary advertising channels
7:4 | RW | BLEM17 | Set default priority value for ISO channel subsequent Tx/Rx attempt
3:0 | RW | BLEM16 | Set default priority value for ISO channel first Tx/Rx attempt

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:28 | BLEMDEFAULT | BLEMDEFAULT_3 |  | 0x3*
11:8 | BLEM18 | BLEM18_2 |  | 0x2*
7:4 | BLEM17 | BLEM17_7 |  | 0x7*
3:0 | BLEM16 | BLEM16_7 |  | 0x7*