### BB_RADIOTXRXTIM1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
22:16 | RW | RFRXTMDA1 | RF Rx test mode delay adjustment for uncoded PHY at 2Mbps
14:8 | RW | RXPATHDLY1 | Rx path delay (in us) for uncoded PHY at 2Mbps
6:0 | RW | TXPATHDLY1 | Rx path delay (in us) for uncoded PHY at 2Mbps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
22:16 | RFRXTMDA1 | RFRXTMDA1_0 |  | 0x0*
14:8 | RXPATHDLY1 | RXPATHDLY1_0 |  | 0x0*
6:0 | TXPATHDLY1 | TXPATHDLY1_0 |  | 0x0*