### BBIF_COEX_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
1 | RW | TX | WLAN collocated device transmit active
0 | RW | RX | WLAN collocated device reception active

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
1 | TX | COEX_TX_IDLE | RF front-end has no non-BLE TX activity | 0x0*
|  | COEX_TX_BUSY | RF front-end performs a non-BLE TX activity | 0x1
0 | RX | COEX_RX_IDLE | RF front-end has no non-BLE RX activity | 0x0*
|  | COEX_RX_BUSY | RF front-end performs a non-BLE RX activity | 0x1