### BB_RADIOTXRXTIM2

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | RXFLUSHPATHDLY2 | Rx path delay (in us) for coded PHY at 125kbps
23:16 | RW | RFRXTMDA2 | RF Rx test mode delay adjustment for uncoded PHY at 125kbps
15:8 | RW | RXPATHDLY2 | Rx path delay (in us) for uncoded PHY at 125kbps
6:0 | RW | TXPATHDLY2 | Rx path delay (in us) for uncoded PHY at 125kbps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | RXFLUSHPATHDLY2 | RXFLUSHPATHDLY2_0 |  | 0x0*
23:16 | RFRXTMDA2 | RFRXTMDA2_0 |  | 0x0*
15:8 | RXPATHDLY2 | RXPATHDLY2_0 |  | 0x0*
6:0 | TXPATHDLY2 | TXPATHDLY2_0 |  | 0x0*