### GPIO_OUTPUT_DATA

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
15:0 | RW | DATA | GPIO[15:0] output data

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
15:0 | DATA | GPIO0_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO1_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO2_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO3_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO4_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO5_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO6_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO7_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO8_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO9_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO10_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO11_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO12_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO13_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO14_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO15_OUT_LOW | Set the GPIO pad to low if IO_MODE is GPIO | 0x0*
|  | GPIO0_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x1
|  | GPIO1_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x2
|  | GPIO2_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x4
|  | GPIO3_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x8
|  | GPIO4_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x10
|  | GPIO5_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x20
|  | GPIO6_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x40
|  | GPIO7_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x80
|  | GPIO8_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x100
|  | GPIO9_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x200
|  | GPIO10_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x400
|  | GPIO11_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x800
|  | GPIO12_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x1000
|  | GPIO13_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x2000
|  | GPIO14_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x4000
|  | GPIO15_OUT_HIGH | Set the GPIO pad to high if IO_MODE is GPIO | 0x8000