### SAU_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
1 | RW | ALLNS | All non-secure
0 | RW | ENABLE | Enable the SAU

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
1 | ALLNS | MEM_AS_SECURE | Memory is marked as Secure and is not Non-secure callable | 0x0*
|  | MEM_AS_NON_SECURE | Memory is marked as Non-secure | 0x1
0 | ENABLE | SAU_DISABLED | The SAU is disabled | 0x0*
|  | SAU_ENABLED | The SAU is enabled | 0x1