### AHBREGS_CHIP_ID_NUM

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | R | CHIP_FAMILY | Chip Family number
23:16 | R | CHIP_VERSION | Chip Version number
15:8 | R | CHIP_MAJOR_REVISION | Chip Major Revision number
7:0 | R | CHIP_MINOR_REVISION | Chip Minor Revision number

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | CHIP_FAMILY | CHIP_FAMILY_NB | BLE family | 0xB*
23:16 | CHIP_VERSION | CHIP_VERSION_NB | Value for Nechako | 0x2*
15:8 | CHIP_MAJOR_REVISION | CHIP_MAJOR_REVISION_NB | Value for Nechako SV2 | 0x2*
7:0 | CHIP_MINOR_REVISION | CHIP_MINOR_REVISION_NB | Value for Nechako SV2 | 0x0*