### DMA_ID_NUM

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
20 | R | DMA_24BIT_WORD | 24-bit word size supported
19:16 | R | DMA_NUMBER | DMA channel number
15:8 | R | DMA_MAJOR_REVISION | DMA Major Revision number
7:0 | R | DMA_MINOR_REVISION | DMA Minor Revision number

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
20 | DMA_24BIT_WORD | DMA_24BIT_WORD_NOT_SUPPORTED | 24-bit word size not supported | 0x0*
|  | DMA_24BIT_WORD_SUPPORTED | 24-bit word size supported | 0x1
15:8 | DMA_MAJOR_REVISION | DMA_MAJOR_REVISION | DMA revision 1.0 | 0x1*
7:0 | DMA_MINOR_REVISION | DMA_MINOR_REVISION | DMA revision 1.0 | 0x0*