## Memory Protection Unit Registers

Register Name | Register Description | Address
--- | --- | ---
MPU_TYPE | Indicates how many regions the MPU for the selected security state supports | 0xE000ED90
MPU_CTRL | MPU control register | 0xE000ED94
MPU_RNR | MPU Region Number Register | 0xE000ED98
MPU_RBAR | MPU Region Base Address Register | 0xE000ED9C
MPU_RLAR | MPU Region Limit Address Register | 0xE000EDA0
MPU_RBAR1 | MPU Region 1 Base Address Register | 0xE000EDA4
MPU_RLAR1 | MPU Region 1 Limit Address Register | 0xE000EDA8
MPU_RBAR2 | MPU Region 2 Base Address Register | 0xE000EDAC
MPU_RLAR2 | MPU Region 2 Limit Address Register | 0xE000EDB0
MPU_RBAR3 | MPU Region 3 Base Address Register | 0xE000EDB4
MPU_RLAR3 | MPU Region 3 Limit Address Register | 0xE000EDB8
MPU_MAIR0 | MPU Memoryattribute Indirection Register 0 | 0xE000EDC0