# Power Modes Registers

Register Name | Register Description | Address
--- | --- | ---
SYSCTRL_WAKEUP_ADDR | Wake-up Restore Address in Unpacked 32-bit Format | 0x4000001C
ACS_PWR_MODES_CTRL | Power Modes Control Register | 0x40001B5C
ACS_SLEEP_MODE_CFG | Sleep power mode configuration | 0x40001B60
ACS_WAKEUP_CTRL | Wake-Up control / Status Register | 0x40001B64
ACS_WAKEUP_CFG | Wake-up Configuration Register | 0x40001B68
ACS_WAKEUP_STATE | RTC Timer wake-up value and wakeup source | 0x40001B6C
ACS_BOOT_CFG | Boot configuration Register | 0x40001B70
ACS_BOOT_GP_DATA | Boot control Register Register | 0x40001B74
ACS_PWR_CTRL | ACS Power Control Register | 0x40001B8C