### BB_FINETIMTGT

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
27:0 | RW | FINETARGET | Fine timer target value on which a ble_finetgtim_irq must be generated (this timer has a precision of 312.5us and interrupt is generated only when FINETARGET = CLKN)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
27:0 | FINETARGET | FINETARGET_0 |  | 0x0*