### RF_REG11

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | FILTER_GAIN_LIN_FILTER | Enable the linear filtering (banked)
30 | RW | FILTER_GAIN_LOW_LIN_GAIN | Reduce the total gain by two if the linear gain is set (banked)
29:27 | RW | FILTER_GAIN_GAIN_M | Mantissa of the final stage gain of the matched filter (banked)
26:24 | RW | FILTER_GAIN_GAIN_E | Exponent of the final stage gain of the matched filter (banked)
23:20 | RW | TX_MULT_TX_MULT_EXP | Exponent of the Tx multiplier (banked)
19:16 | RW | TX_MULT_TX_MULT_MAN | Mantissa of the Tx multiplier (banked)
15:12 | RW | TX_FRAC_CONF_TX_FRAC_DEN | Denominator of the fractional data-rate in Tx mode (banked)
11:8 | RW | TX_FRAC_CONF_TX_FRAC_NUM | Numerator of the fractional data-rate in Tx mode (banked)
7:4 | RW | RX_FRAC_CONF_RX_FRAC_DEN | Denominator of the fractional data-rate in Rx mode (banked)
3:0 | RW | RX_FRAC_CONF_RX_FRAC_NUM | Numerator of the fractional data-rate in Rx mode (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | FILTER_GAIN_LIN_FILTER | FILTER_GAIN_LIN_FILTER_DISABLE | Disable the linear filtering | 0x0*
|  | FILTER_GAIN_LIN_FILTER_ENABLE | Enable the linear filtering | 0x1
30 | FILTER_GAIN_LOW_LIN_GAIN | FILTER_GAIN_LOW_LIN_GAIN_DISABLE | Disable total gain reduction | 0x0*
|  | FILTER_GAIN_LOW_LIN_GAIN_ENABLE | Enable total gain reduction | 0x1
29:27 | FILTER_GAIN_GAIN_M | FILTER_GAIN_GAIN_M_DEFAULT |  | 0x0*
26:24 | FILTER_GAIN_GAIN_E | FILTER_GAIN_GAIN_E_DEFAULT |  | 0x0*
23:20 | TX_MULT_TX_MULT_EXP | TX_MULT_TX_MULT_EXP_DEFAULT |  | 0x2*
19:16 | TX_MULT_TX_MULT_MAN | TX_MULT_TX_MULT_MAN_DEFAULT |  | 0x9*
15:12 | TX_FRAC_CONF_TX_FRAC_DEN | TX_FRAC_CONF_TX_FRAC_DEN_DEFAULT |  | 0x0*
11:8 | TX_FRAC_CONF_TX_FRAC_NUM | TX_FRAC_CONF_TX_FRAC_NUM_DEFAULT |  | 0x0*
7:4 | RX_FRAC_CONF_RX_FRAC_DEN | RX_FRAC_CONF_RX_FRAC_DEN_DEFAULT |  | 0x0*
3:0 | RX_FRAC_CONF_RX_FRAC_NUM | RX_FRAC_CONF_RX_FRAC_NUM_DEFAULT |  | 0x0*