### TIMER_ID_NUM

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
20 | R | TIMER_GPIO_CAP | Implementation of the GPIO triggered capture
19:16 | R | TIMER_ID_NUM | TIMER instance number
15:8 | R | TIMER_MAJOR_REVISION | TIMER Major Revision number
7:0 | R | TIMER_MINOR_REVISION | TIMER Minor Revision number

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
20 | TIMER_GPIO_CAP | TIMER_GPIO_CAP_DISABLED | GPIO capture is not implemented | 0x0*
|  | TIMER_GPIO_CAP_ENABLED | GPIO capture is implemented | 0x1
15:8 | TIMER_MAJOR_REVISION | TIMER_MAJOR_REVISION | Timer revision 1.0 | 0x1*
7:0 | TIMER_MINOR_REVISION | TIMER_MINOR_REVISION | Timer revision 1.0 | 0x0*